|  |
| --- |
| ` |
| ބީލަން ފޮތް |
| **ޕްރޮޖެކްޓްގެ ނަން: ޑާޓާ ސެންޓަރ އަޕްގުރޭޑުކުރުން****ޕްރޮޖެކްޓް ނަންބަރު: 22PU-2022-G-18****އިޢުލާން ނަންބަރު: (IUL)22-PU/22/2022/337** |
|  **14 ނޮވެންބަރު 2022** |

|  |
| --- |
| **މިނިސްޓްރީ އޮފް އެޑިޔުކޭޝަން****މާލެ، ދިވެހިރާއްޖެ** |

|  |
| --- |
| **ސެކްޝަން 1**  |
| **ބީލަން ޝީޓް** |
|

|  |
| --- |
|  |
| **ބީލަމާއި ގުޅޭ ރިފަރަންސްތައް** | **ރިފަރަންސް ނަންބަރު** |
| މަސައްކަތުގެ ނަން: **ޑާޓާ ސެންޓަރ އަޕްގުރޭޑުކުރުން**އިޢުލާން ނަންބަރު: **(IUL)22-PU/22/2022/337**އިޢުލާން ކުރި ތާރީޚް:  **14 ނޮވެންބަރު 2022** | 1.1 |
| ބީލަން ހުށަހެޅުމަށް ރަޖިސްޓްރީކުރުން:**"ބިޑް ރަޖިސްޓްރީ ފޯމް"** **ގެ ލިންކު:** <https://forms.moe.gov.mv>މުއްދަތު: **2022 ނޮވެންބަރު 14 ން 2022 ނޮވެންބަރު 19 ގެ ނިޔަލަށް** | 8.1 |
| ޕްރީ ބިޑް މީޓިންގ އޮންނާނެ ތަނާއި ތާރީޚްތަން: -ތާރީޚް: -ދުވަސް: - ގަޑި: - | 9.1 |
| މަޢުލޫމާތު ސާފުކުރުމަށް ލިޔުންތައް ފޮނުވަންވީ އެޑްރެސް:އޮފީސް: މިނިސްޓްރީ އޮފް އެޑިޔުކޭޝަން/ޕްރޮކިއުމަންޓް ސެކްޝަންގުޅޭނެ ނަންބަރު: 3341403އީމެއިލް އެޑްރެސް: procurement@moe.gov.mv  | 9.2 |
| އަގު ހުށަހަޅަންވީ ގޮތް: ސެކްޝަން-7 ގައިވާ މަޢުލޫމާތާ އެއްގޮތަށް އަގު ކޯޓޭޝަންގައި ހުށަހެޅުމަށް | 13.1 |
| މަސައްކަތުގެ މުއްދަތު:ސެކްޝަން-7 ގައިވާ މަޢުލޫމާތާ އެއްގޮތަށް މުއްދަތު ހުށަހެޅުމަށް | 14 |
| ބީލަން ހުށަހަޅަންވީ ސުންގަޑިތަން: މިނިސްޓްރީ އޮފް އެޑިޔުކޭޝަން / ވެލާނާގެ 9 ވަނަ ފަންގިފިލާ / މީޓިންގ ރޫމް 03 ތާރީޚް: **22 ނޮވެންބަރު 2022**ދުވަސް: އަންގާރަގަޑި: **11:00** | 18.1 |
| ބީލަން ހުޅުވުންތަން: މިނިސްޓްރީ އޮފް އެޑިޔުކޭޝަން / ވެލާނާގެ 9 ވަނަ ފަންގިފިލާ / މީޓިންގ ރޫމް 03 ތާރީޚް: **22 ނޮވެންބަރު 2022**ދުވަސް: އަންގާރަގަޑި: **11:00** | 20.1 |
| ބީލަންތައް ވަޒަންކުރާނެ މިންގަނޑު ޖަދުވަލު 6 ގައި އެވަނީއެވެ. | 24.1 |
| ބިޑް ސެކިއުރިޓީގެ ގޮތުގައި ހުށަހަޅަންޖެހޭ އަދަދު: **50,000/- (ފަންސާސް ހާސް) ރުފިޔާ** | 28.1 |
| ބިޑް ސެކިއުރިޓީގެ މުއްދަތަކީ ބިޑް ހުޅުވާ ދުވަހުން ފެށިގެން 60 (ފަސްދޮޅަސް) ދުވަހެވެ. | 28.2 |
| ޕާރފޯމަންސް ގެރެންޓީ ހުށަހަޅަންޖެހޭ އަދަދު: **ހުށަހަޅާ އަގުގެ 5%(ބީލަން ކާމިޔާބުކުރާ ފަރާތުން)** | 30.1 |

 |
|  |
| **ސެކްޝަން 2 - ބީލަށް ހުށަހަޅާ ފަރާތްތަކަށްދެވޭ އިރުޝާދު** |
| **(ހ) އާންމު މަޢުލޫމާތު** |
| 1. **ބީލަމުގެ ތަޢާރަފު**
 |  | މި ބީލަމަކީ ބީލަން ޝީޓުގައި ބަޔާންކޮށްފައިވާ ޚިދުމަތް ނުވަތަ ތަކެތި ފޯރުކޮށްދޭނެ ފަރާތެއް ހޯދުމަށް ހުޅުވާލެވިފައިވާ ބީލަމެކެވެ. މި ބީލަމުން ހޯދަންބޭނުންވާ ޚިދުމަތް ނުވަތަ މަސައްކަތުގެ މަޢުލޫމާތު ބީލަން ޝީޓުގައި ބަޔާންކޮށްފައިވާނެއެވެ. |
| 1. **ބީލަމަށް ކުރިމަތިލެވޭނެ ފަރާތްތައް**
 |  | ބީލަން ހުޅުވާލެވިފައިވަނީ، ވިޔަފާރި ރަޖިސްޓުރީ ކުރުމުގެ ޤާނޫނު (ޤާނޫނު ނަންބަރ: 18/2014) ގެ ދަށުން ވިޔަފާރި ރަޖިސްޓުރީ ކުރެވިފައިވާ ތިރީގައި ބަޔާންކުރާ ފަރާތްތަކަށެވެ.  |
|  | 2.1.1 ދިވެހިރާއްޖޭގެ ކުންފުންޏާބެހޭ ޤާނޫނުގެ ދަށުން ރަޖިސްޓުރީ ކުރެވިފައިވާ ކުންފުނިތައް. |
|  | 2.1.2 ޕާޓްނަރޝިޕް ޤާނޫނުގެ ދަށުން ރަޖިސްޓްރީ ކުރެވިފައިވާ ޕާޓްނަރޝިޕްތައް. |
|  |  | 2.1.3 ކޯޕަރޭޓިވް ސޮސައިޓީގެ ޤާނޫނުގެ ދަށުން ރަޖިސްޓްރީ ކުރެވިފައިވާ ކޯޕަރޭޓިވް ސޮސައިޓީތައް. |
|  |  | 2.1.4 އަމިއްލަ ފަރުދުންގެ ވިޔަފާރީގެ ޤާނޫނުގެ ދަށުން ރަޖިސްޓްރީ ކުރެވިފައިވާ އަމިއްލަ ފަރުދުންގެ ވިޔަފާރިތައް. |
|  |  | މިމާއްދާގައި ބަޔާންކުރާ ފަރާތްތަކުގެ އިތުރުން އެހެން ފަރާތްތަކަކަށް ބީލަމަށް ކުރިމަތިލެވޭނަމަ އެކަން ބީލަން ޝީޓްގައި ބަޔާން ކޮށްފައިވާނެއެވެ. |
| 1. **ބީލަން އޮންނަންވާނެގޮތާއި ބީލަމުގައި ސޮއިކުރުން**
 |  | ބީލަންތައް އޮންނަންވާނީ މި ލިޔުމުގެ އެނެކްސް 1 ގައިވާ، ބީލަން ހުށަހަޅާ ފަރާތްތަކުގެ ޗެކުލިސްޓު ގައިވާ ލިއުންތަކާއި ޑޮކިއުމަންޓުތައް ހިމެނޭގޮތަށް ތަރުތީބުން ބައިންޑު ކުރެވިފައެވެ. |
|  | ބީލަން އޮންނަންވާނީ ދިވެހިބަހުން ނުވަތަ އިގިރޭސި ބަހުން، ފަސޭހައިން ކިޔަން އެނގޭ ފޮންޓަކުން (ފަރުމާ ފޮންޓް ފަދަ) ޓައިޕު ކުރެވިފައެވެ. ނުވަތަ އަތުން ލިޔާނަމަ ލިޔެފައި ހުންނަންވާނީ ކިޔަން އެނގޭގެ ގޮތަށެވެ. އަދި ބީލަމުގެ ހުރިހާ ސަފްހާއެއްގައި ބީލަން ހުށަހަޅާ ފަރާތުގެ ނުވަތަ އެފަރާތުން އައްޔަން ކުރާ ފަރާތުގެ ސޮޔާއި ތައްގަނޑު ޖަހާފައި އޮންނަން ވާނެއެވެ. އަދި ބީލަމުގެ ކޮންމެ ޞަފުޙާއެއްގައި ވެސް އެއީ ކިތައް ޞަފުހާގެ ތެރެއިން ކިތައް ވަނަ ޞަފުޙާކަން އެނގޭގޮތަށް ތަރުތީބުން ޞަފުޙާ ނަންބަރުވެސް ޖަހަންވާނެއެވެ. |
|  | 3.3.1 ޕްރައިވެޓް ލިމިޓެޑް ކުންފުނިތަކުން މެނޭޖިންގ ޑިރެކްޓަރ ނޫން އެހެން ފަރާތަކުން ބީލަމުގައި ސޮއިކުރާނަމަ އެ ފަރާތަކަށް ސޮއި ކުރުމުގެ ހުއްދަ ދެވިފައިވާކަން ބަޔާންކުރާ "ޕަވަރ އޮފް އެޓާރނީ"ގެ ކޮޕީއެއް ހުށަހަޅަން ވާނެއެވެ. 3.3.2 ޕާޓްނަރޝިޕްތަކުގެ މެނޭޖިންގ ޕާޓްނަރު ނޫން އެހެން ފަރާތަކުން ބީލަމުގައި ސޮއިކުރާނަމަ އެ ފަރާތަކަށް ސޮއި ކުރުމުގެ ހުއްދަ ދެވިފައިވާކަން ބަޔާންކުރާ "ޕަވަރ އޮފް އެޓާރނީ"ގެ ކޮޕީއެއް ހުށަހަޅަން ވާނެއެވެ.3.3.2 ކޯޕަރޭޓިވް ސޮސައިޓީތަކުގެ ޗެއަރޕާރސަން ނޫން އެހެން ފަރާތަކުން ބީލަމުގައި ސޮއިކުރާނަމަ އެ ފަރާތަކަށް ސޮއި ކުރުމުގެ ހުއްދަ ދެވިފައިވާކަން ބަޔާންކުރާ "ޕަވަރ އޮފް އެޓާރނީ"ގެ ކޮޕީއެއް ހުށަހަޅަން ވާނެއެވެ.3.3.4 ފަރުދީ ވިޔަފާރިތަކުގައި ވެރިފަރާތް ނޫން ފަރާތެއް ބީލަމަށް ހުށަހަޅާ ލިޔުންތަކުގައި ސޮއިކުރާނަމަ އެފަރާތަކަށް ސޮއިކުރުމުގެ ހުއްދަ ދެވިފައިވާކަން ބަޔާންކުރާ "ޕަވަރ އޮފް އެޓާރނީ"ގެ ކޮޕީއެއް ހުށަހަޅަން ވާނެއެވެ. |
|  |  | 3.3.5 ސަރުކާރު ކުންފުނިތަކާއި، ޕަބްލިކް ލިމިޓެޑް ކުންފުނިތަކުން ބީލަމުގެ ލިޔުންތަކުގައި ސޮއިކުރާއިރު، ޒިންމާދާރު ކޮންމެފަރާތަކަށްވެސް ސޮއި ކުރެވިދާނެއެވެ. |
| 1. **ހުށަހެޅޭނެ ބީލަމުގެ އަދަދު**
 |  | ބީލަމަށް ކުރިމަތިލާ ކޮންމެ ފަރާތަކަށްވެސް ހުށަހެޅޭނީ 1 (އެކެއް) ބީލަމެވެ. އެއް ބީލަމަށްވުރެ ގިނަ ބީލަށް އެއްވެސް ފަރާތަކުން ހުށަހަޅާފިނަމަ އެފަރާތުން ހުށަހަޅާގައިވާ ހުރިހާ ބީލަމެއް ބާތިލް ކުރެވޭނެއެވެ. |
| 1. **ބީލަން ތައްޔާރު ކުރުމުގެ އަގު**
 |  | ބީލަން ތައްޔާރުކުރުމަށާއި ބީލަން ހުށަހެޅުމަށް ކުރާ އެންމެހައި ޚަރަދެއް ކުރާނީ އެބީލަމެއް ހުށަހަޅާ ފަރާތަކުންނެވެ. މިކަމަށް ހިނގާ އެއްވެސް ޚަރަދަކަށް ބީލަމަށް ހުޅުވާލި ފަރާތުން ޒިންމާއެއް ނުނަގާނެއެވެ. |
| 1. **އެހެނިހެން އުސޫލްތައް**
 |  | ބީލަން ހުށަހަޅާ ފަރާތަކީ، މިނިސްޓްރީ އޮފް އެޑިޔުކޭޝަނާއި، މިނިސްޓްރީގެ ދަށުން ހިނގަމުންދާ އެއްވެސް އިދާރާއެއްގެ ވެރިއެއް ނުވަތަ މުވައްޒަފަކާ ތިމާގެކަމުގެ ނުވަތަ ވިޔަފާރީގެ އެއްވެސް ގުޅުމެއް އޮތް ފަރާތެއް ކަމުގައިވާނަމަ ނުވަތަ މި މިނިސްޓްރީގެ ދާއިރާގެ އެއްވެސް އޮފީހެއްގައި ވަޒީފާ އަދާކުރާ ފަރާތެއް ނަމަ އެކަމުގެ ސާފު މަޢުލޫމާތު އެނގޭނެ ލިޔުމެއްގައި ސޮއިކޮށް ހުށަހަޅަންވާނެއެވެ. މިފަދަ ލިޔުމެއް ހުށަނާޅާ ހުއްޓާ އެކަން އެނގިއްޖެނަމަ އިތުރު އެންގުމަކާ ނުލައި އެ ބީލަން ބާތިލް ކުރެވޭނެއެވެ. |
| **(ށ) ބީލަމާގުޅޭ ލިޔުންތައް** |
| 1. **ބީލަން ފޮތު ގައި ހިމެނޭ ބައިތައް**
 |  | ބީލަމާގުޅޭ ލިޔުންތަކުގައި ހިމެނެނީ ތިރީގައިވާ ލިސްޓްގައިވާ ލިޔުންތަކާއި، އެމެންޑްމަންޓްތަކެވެ. |
|  | 7.1.1 ބީލަން ޝީޓް (ސެކްޝަން-1) |
|  |  7.1.2ބީލަށް ހުށަހަޅާ ފަރާތްތަކަށްދެވޭ އިރުޝާދު (ސެކްޝަން-2) |
|  |  | 7.1.3 އެއްބަސްވުމުގެ އާންމު އަދި ހާއްސަ މާއްދާތައް (ސެކްޝަން-3) |
|  |  | 7.1.4 ޖަދުވަލުތައް (ސެކްޝަން-4) |
|  |  | 7.1.5 ކޮންޓްރެކްޓް ޑާޓާ ޝީޓް (ސެކްޝަން - 5 ) |
|  |  | 7.1.6 އެއްބަސްވުން (ސެކްޝަން -6 ) |
|  |  |  7.1.7 މަސައްކަތާބެހޭ މަޢުލޫމާތު (ސެކްޝަން–7 ) |
| 1. **ބީލަމުގައި ރަޖިސްޓްރީ ކުރުން**
 |  | ބީލަމުގައި ބައިވެރިވުމަށް އިޢުލާނުގައިވާ މުއްދަތުގެ ތެރޭގައި އިޢުލާނުގައި ދީފައިވާ އިރުޝާދާ އެއްގޮތަށް ރަޖިސްޓްރީ ކުރަންވާނެއެވެ. |
|  | ބީލަން ހުށަހެޅޭނީ އިޢުލާނުގައި ރަޖިސްޓަރީ ކުރުމަށް ދެވިފައިވާ މުއްދަތުގެ ތެރޭގައި ރަޖިސްޓްރީކުރާ ފަރާތްތަކަށެވެ. |
|  |  | ބީލަމުގައި ރަޖިސްޓްރީކުރުމަށް ދީފައިވާ މުއްދަތުގެ ތެރޭގައި ރަޖިސްޓްރީ ސިސްޓަމަށް ދިމާވާ މައްސަލައަކާ ގުޅިގެން ރަޖިސްޓްރީ ނުކުރެވޭނަމަ، ރަޖިސްޓްރޭޝަންގެ މުއްދަތު ހަމަވުމުގެ ކުރިން އިޢުލާންގައިވާ އީމެއިލް އެޑްރެހަށް އެކަން ބަޔާންކޮށް ހުށަހެޅުމުން ރަޖިސްޓްރީކޮށްދެވޭނެއެވެ. |
| 1. **ބީލަމާ ގުޅޭގޮތުން މައުލޫމާތު ސާފުކުރުން**
 |  | މި ބީލަމާއި ގުޅޭ ޕްރީބިޑް މީޓިން އެއް ބާއްވާނަމަ، ޕްރީބިޑް މީޓިން އޮންނާނެ ތާރީޚާއި ގަޑި "ބީލަން ޝީޓް" ގައި ބަޔާންކޮށްފައިވާނެއެވެ. |
|  | ބީލަމާގުޅޭގޮތުން އިތުރު މަޢުލޫމާތެއް ސާފުކުރަން ބޭނުންވާނަމަ ބީލަން ޝީޓްގައިވާ އެޑްރެހަށް ލިޔުމުން ހުށަހެޅުމުން، އެކަމުގެ މަޢުލޫމާތު ސާފުކޮށްދިނުމަށްފަހު ހުރިހާ ބީލަންވެރިންނަށް ލިޔުމުން ފޮނުވޭނެއެވެ. |
|  | މި ބީލަން ފޮތުގައިވާ މަޢުލޫމާތާއި ގުޅިގެން ނުވަތަ މި ބީލަމާ ގުޅޭގޮތުން އިތުރަށް ސާފުނުވާ ކަމެއް އޮތް ނަމަ އެ ކަމެއްގެ މައުލޫމާތު ހޯދުމަކީ ބީލަން ހުށަހަޅާ ފަރާތުގެ ޒިންމާ އެކެވެ. |
| 1. **ބީލަމަށް ބަދަލު ގެނައުން**
 |  | ބީލަން ހުޅުވުމުގެ މުއްދަތު ހަމަވުމުގެ ކުރިން ބީލަމަށް ކޮންމެހެން ގެންނަންޖެހޭ ބަދަލެއް ގެނައުމަށް ފެނިއްޖެ ހިދެއްގައި، އެމެންޑްމަންޓެއް (އުނި/އިތުރު) ގެނެވޭނެއެވެ.  |
|  |  | 0.11 ގައިވާ ގޮތަށް ދޫކުރާ އެމެންޑްމަންޓަކީ ބީލަމުގެ ބައެކެވެ. އަދި އެ އުނިއިތުރު ބީލަމުގެ މަޢުލޫމާތު ސާފުކުރުމަށް ޙާޟިރުވި ފަރާތްތަކަށް އީމެއިލް މެދުވެރިކޮށް ފޮނުވަންވާނެއެވެ.  |
| **(ނ) ބީލަން ތައްޔާރުކުރުން** |
| 1. **ބީލަމުގައި ބޭނުން ކުރެވޭ ބަސް**
 |  | ބީލަން ހުށަހަޅާ ފަރާތުން ބީލަން ތައްޔާރު ކުރަންވާނީ ބީލަމާއިއެކު ދީފައިވާ ނަމޫނާއާ އެއްގޮތަށް ދިވެހިބަހުންނެވެ. އަދި ބީލަމާއިއެކު ހުށަހަޅަންޖެހޭ ރިފަރެންސް ލިޔުންތައް އިގިރޭސި ބަހުން ހުށަހެޅިދާނެއެވެ.  |
| 1. **ބީލަމުގައި ބޭނުން ކުރާ ފައިސާ**
 |  | މި ބީލަމުގައި އަގު ކުރެވިފައި ހުންނަންވާނީ ދިވެހި ރުފިޔާއިންނެވެ.  |
| 1. **އަގު ހުށަހެޅުން**
 |  | ބީލަމަށް ވަކި ގޮތަކަށް އަގު ހުށަހަޅަންޖެހޭނަމަ އެކަން ބީލަން ޝީޓްގައި ބަޔާންކޮށްފައިވާނެއެވެ. |
|  |  | ޖީ.އެސް.ޓީއަށް ރަޖިސްޓްރީކޮށްފައިވާ ފަރާތެއްނަމަ އަގު ހުށަހަޅަންވީ ޖީ.އެސް.ޓީ ހިމަނައިގެންނެވެ. އަދި ޖީ.އެސް.ޓީއަށް ދައްކާ އަދަދު ވަކިން އެނގެން އޮންނަންވާނެއެވެ. |
| 1. **މުއްދަތު**
 |  | މަސައްކަތްކޮށްދިނުމަށް މުއްދަތު ހުށަހަޅަންޖެހޭނީ ބަންދު ދުވަސްތައް ހިމަނައިގެން ދުވަހުގެ އަދަދުންނެވެ. |
|  |  | މަސައްކަތްކޮށްދިނުމަށް ހުށަހަޅާ މުއްދަތަކީ އެމަސައްކަތެއް ކުރުމަށް އެކަށީގެންވާ މުއްދަތެއް ކަމުގައި ވާންވާނެއެވެ. |
|  |  | ވަކިމުއްދަތަކަށް ނިންމުމަށް ކަނޑައަޅާފައިވާ މަސައްކަތެއްނަމަ، އެމަސައްކަތެއް އެމުއްދަތަށް މަސައްކަތް ނިންމަންވާނެއެވެ. |
| 1. **ބީލަމުގެ މުއްދަތު**
 |  | ބީލަމުގެ މުއްދަތު ހަމަވާ ތާރީޚް އޮންނަންވާނީ ބީލަން ހުށަހަޅާ ތާރީޚުން ފެށިގެން މަދުވެގެން 60 ދުވަސް ދުވަހުގެ މުއްދަތަށެވެ. |
| 1. **ބީލަމާއެކު ހުށަހަޅަންޖެހޭ ލިޔުންތައް**
 |  | ބީލަން ހުށަހަޅާއިރު ތިރީގައިމިވާ މަޢުލޫމާތު އަދި ލިޔުމެއް އަދި ލިޔުންތައް މަދު ނުވަތަ ނެތްނަމަ ޑިސްކޮލިފައި ކުރެވޭނެއެވެ.  |
|  | 16.1.1 ފުރިހަމަ ކޮށްފައިވާ ބީލަން ހުށަހަޅާ ފޯމް (ޖަދުވަލު 2 ) |
|  | 16.1.2 ކުންފުނި/ޕާޓްނަރޝިޕް/ ކޯޕަރޭޓިވް ސޮސައިޓީ/ އަމިއްލަ ފަރުދުންގެ ވިޔަފާރީގެ ރެޖިސްޓްރީގެ ކޮޕީ. |
|  | 16.1.3 ކޯޓޭޝަން/ ބީ.އޯ.ކިޔު (ހުށަހަޅަންޖެހޭނެ ކަމަށް ބީލަން ޝީޓްގައި ބުނެފައިވާނަމަ ހުށަހަޅަންޖެހޭނެއެވެ.) |
|  |  | 16.1.4 ފުރިހަމަކޮށްފައިވާ ބީލަން ހުށަހަޅާ ފަރާތުގެ ޕްރޮފައިލް (ޖަދުވަލު 3) |
|  |  | 16.1.5 ޖީ.އެސް.ޓީ ރެޖިސްޓްރޭޝަން ސެޓްފިކެޓްގެ ކޮޕީ (ޖީ.އެސް.ޓީއަށް ރެޖިސްޓްރީކޮށްފައިވާނަމަ) |
|  |  | 16.1.6 ބިޑް ސެކިއުރިޓީ ހުށަހަޅަންޖެހޭ ބީލަމެއްނަމަ ހުށަހަޅާ ބިޑް ސެކިއުރިޓީ |
|  |  | 16.1.7 ސްޕެސިފިކޭޝަން ފޯމް (ޖަދުވަލު - 9) (ބީލަމުގައި ހުށަހަޅަންޖެހޭނެ ކަމަށް ބަޔާންކުރާނަމަ) |
|  |  |  16.1.8ހުށަހަޅާ ޓެކްނިކަލް ޓީމްގެ މަޢުލޫމާތު، ސީ.ވީ، އެކްރެޑިޓެޑް ސެޓްފިކެޓްތައް. |
|  |  | ބީލަން ހުށަހަޅާއިރު ތިރީގައިމިވާ މަޢުލޫމާތު އަދި ލިޔުމެއް އަދި ލިޔުންތައް މަދު ނުވަތަ ނެތްނަމަ މާރކްސް ނުލިބޭނެއެވެ. |
|  |  | 16.2.1 ބީލަން ހުށަހަޅާ މަސައްކަތާގުޅުންހުރި މަސައްކަތުގެ ތަޖްރިބާގެ ލިޔުންތައް އަދި ޖަދުވަލު 5 ފުރިހަމަ ކުރުމަށްފަހު ހުށަހަޅަންވާނެއެވެ. |
|  |  | 16.2.2 ބީލަން ހުށަހަޅާ ފަރާތުގެ މާލީ ދަލީލު އަދި ޖަދުވަލު 4 ފުރިހަމަ ކުރުމަށްފަހު ހުށަހަޅަންވާނެއެވެ. |
|  |  | (ހ) ބޭންކް ރިފަރެންސް ލެޓަރ ނުވަތަ ސްޓޭޓްމަންޓްގައިވާ އެކައުންޓްގެ ވެރިފަރާތަކީ ބީލަމުގައި ރަޖިސްޓްރީކޮށްފައިވާ ފަރާތްކަމުގައި ވާންޖެހޭނެއެވެ. |
|  |  | (ށ) އަމިއްލަ ފަރުދުންގެ ވިޔަފާރީގެ ދަށުން ބީލަން ހުށަހަޅާނަމަ، އެފަރާތުގެ އަމިއްލަ ނަމުގައި ހުޅުވާފައިވާ އެކައުންޓްގެ ބޭންކް ރެފަރެންސް ލެޓަރ ނުވަތަ ސްޓޭޓްމަންޓްވެސް ގަބޫލުކުރެވޭނެއެވެ. |
|  |  | (ނ) ފާއިތުވި މަހުގެ ބޭންކް ބެލެންސް އަދަދު އިނގޭނެހެން ބޭންކް ރިފަރެންސް ސިޓީ އެއް ނުވަތަ ބޭންކު ސްޓޭޓްމަންޓް ހުށަހަޅަންވާނެއެވެ. |
|  |  | 16.2.3 ކްރެޑިޓް ރެފަރެންސް ސިޓީތައް. ހުށަހަޅާ ކްރެޑިޓް ރެފަރެންސް ސިޓީތަކުގައި ތިރީގައިވާ ޝަރުތުތައް ހަމަވާންޖެހޭނެއެވެ. |
|  |  | (ހ) ރަޖިސްޓްރީކޮށްފައިވާ މާލީ އިދާރާއަކުން ދޫކޮށްފައިވާ ލިއުމެއްކަމުގައި ވާންވާނެއެވެ. |
|  |  | (ށ) ހުށަހެޅޭ ކްރެޑިޓް ރެފަރެންސް އަކީ ޚާއްސަކޮށް މިޕްރޮޖެކްޓަށް ދޫކުރެވިފައިވާ ސިޓީއެއްކަމުގައި ވާންވާނެއެވެ. |
|  |  | (ނ) މިރެފަރަންސްގައި ޕްރޮޖެކްޓްގެ ނަން، ފައިސާގެ/ ކްރެޑިޓްގެ ޢަދަދު، ސިޓީ ދޫކުރެވުނު ތާރީޚް، ކްރެޑިޓްގެ ސިޓީގެ މުއްދަތު ހަމަވާނެ ތާރީޚް އަދި ރެފަރަންސް ދޫކުރާ ފަރާތުގެ ނަމާއި ސޮއި އަދި ސްޓޭމްޕް ސާފުކޮށް އެނގެން އޮންނަންވާނެއެވެ. |
|  |  | (ރ) މިރެފަރަންސް ވާންވާނީ ރެފަރަންސް ދޫކުރިފަރާތުން ދޫކޮށްފައިވާ އޮރިޖިނަލް ރެފަރަންސްއަކަށެވެ. މިފަދަ ރެފަރަންސްތަކުގެ ކޮޕީ ބަލައެއް ނުގަނެވޭނެއެވެ. |
|  |  | (ބ) އަމިއްލަ ފަރުދުން ދޫކޮށްފައިވާ ކްރެޑިޓް ރިފަރެންސް ބަލައެއްނުގަނެވޭނެއެވެ. |
|  |  | އެންމެ ކުދި، ކުދި އަދި މެދުފަންތީގެ ވިޔަފާރިއެއްގޮތުގައި ރަޖިސްޓްރީކޮށްފައިވާނަމަ، ރަޖިސްޓްރީގެ ކޮޕީ. |
|  | * 1. 1
 | އެއްބަސްވުމުގައި ސޮއިކުރުމުގެ ކުރިން ހުށަހަޅަންޖެހޭ ލިޔުންތައް |
|  |  | 16.3.1 މޯލްޑިވްސް އިންލަންޑް ރެވެނިއު އޮތޯރިޓީން ދޫކުރާ ޓެކްސް ކްލިއަރެންސް ރިޕޯޓްގެ ކޮޕީ (ދޫކުރިފަހުން 3 މަސް ހަމަނުވާ) |
|  |  | 16.3.2 ގަވާއިދުން ޕެންޝަން ފައިސާ ދައްކާކަމުގެ ލިޔުމުގެ ކޮޕީ (މުވައްޒަފުންނެތްނަމަ ނެތްކަމަށް ޕެންސަން އޮފީހުންދީފައިވާ ލިޔުން) (ދޫކުރިފަހުން 3 މަސް ހަމަނުވާ).  |
| **(ރ) ބީލަން ހުށަހެޅުން** |
| 1. **ބީލަން ބަންދު ކުރާނެ ގޮތް**
 |  | ބީލަން އޮންނަންވާނީ ބަންދު ކުރެވިފައެވެ. މިނޫންގޮތަކަށް އޮންނަ ބީލަމެއް ބަލައެއް ނުގަނެވޭނެއެވެ.  |
|  |  | ސިޓީ އުރައިގެ ބޭރުގައި ބީލަމުގެ ނަން ލިޔެފައި އޮންނަންވާނެއެވެ.  |
|  |  | ސިޓީ އުރައިގައި ބީލަން ހުށަހަޅާ ފަރާތުގެ ނަމާއި އެޑްރެސް އަދި ފޯނު ނަމްބަރު ލިޔެފާ އޮންނަން ވާނެއެވެ. |
|  |  | ހުށަހަޅާ ބީލަންތައް ހުންނަންވާނީ ބަންދު ކުރެވިފައިވާ ސިޓީ އުރައިގައި ބީލަން ޝީޓްގައިވާ ގޮތަށް އެޑްރެސް ކުރެވިފައެވެ. |
| 1. **ބީލަން ހުށަހެޅުމުގެ ސުންގަޑި**
 |  | މި މަސައްކަތަށް ނުވަތަ ޚިދުމަތަށް އެދި ހުށަހަޅާ ބީލަންތައް ހުށަހަޅަންވީ ސުން ގަނޑި ބީލަން ޝީޓްގައި ބަޔާންކޮށްފައިވާނެއެވެ. |
|  | މި މާއްދާގެ 18.1 ގައި ބަޔާން ކުރެވިފައިވާ ތާރީޚަކީ ސަރުކާރު ބަންދު ދުވަހެއްގެ ގޮތުގައި ސަރުކާރުން ހަމަޖައްސައިފިނަމަ ބީލަން ހުށަހަޅަންޖެހޭ އެންމެފަހު ތާރީޚަކަށް ވާނީ ޖެހިގެން އެންމެ އަވަހަށް އަންނަ ރަސްމީ ދުވަހެއްގެ ބީލަން ޝީޓްގައިވާ ގައިވާ ސުންގަޑީގައެވެ. |
|  |  | އީމެއިލް އަދި ފެކްސް އިން ފޮނުވާ ބީލަންތައް ބަލައެއް ނުގަނެވޭނެއެވެ. |
| 1. **މުއްދަތުގެ ފަހުން ހުށަހެޅޭ ބީލަން ތަކާއި މެދު އަމަލު ކުރާނެގޮތް:**
 |  | ބީލަން ހުށަހެޅުމަށް ހަމަޖެހިފައިވާ ސުންގަޑީގެ ފަހުން ހުށަހަޅާ ބީލަންތައް ބަލައެއް ނުގަނެވޭނެއެވެ. |
| **(ބ) ބީލަން ހުޅުވުމާއި އިވޭލުއޭޓް ކުރުން** |
| 1. **ބީލަން ހުޅުވުން**
 |  | މި މަސައްކަތަށް ހުށަހަޅާ ބީލަންތައް ހުޅުވުމަށް ހަމަޖެހިފައި ވަނީ ބީލަން ހުށަހަޅާ ފަރާތްތަކުގެ ނުވަތަ އެފަރާތުން ބީލަން ހުޅުވުމަށް ހަމަޖެހިފައިވާ ތަނަށް ފޮނުވާ ފަރާތެއްގެ ހާޒިރުގައި ބީލަން ޝީޓްގައިވާ ތާރީޚްގައެވެ. |
|  |  | ބީލަން ހުޅުވުން އޮންނާނީ ބީލަން ޝީޓްގައި ބަޔާންކޮށްފައިވާ އެޑްރެހުގައެވެ. |
|  |  | ބީލަން ހުޅުވުމަށް ހަމަޖައްސާފައިވާ ތާރީޚަކީ އެއްވެސް ސަބަބަކާ ހުރެ ސަރުކާރުން ބަންދު ދުވަހެއްގެ ގޮތުގައި ހަމަޖައްސައިފިނަމަ ބީލަން ހުޅުވުން އޮންނާނީ ޖެހިގެން އަންނަ ރަސްމީ ދުވަހުގެ ބީލަން ޝީޓްގައިވާ ގައިވާ ސުންގަޑީގައެވެ. |
| 1. **ހުށަހަޅާ ބީލަމުގައިވާ ކުށްތައް އިސްލާޚްކުރުން**
 |  | ޝަރުތު ފުރިހަމަވާ ބީލަންތަކުގެ ހިސާބުކުރުމުގެ މައްސަލައެއް އުޅޭނަމަ ތިރީގައި މިވާ ގޮތްތަކުގެ މަތިން އިސްލާޚް ކުރެވޭނެއެވެ. |
|  | ބީލަމުގައިވާ ފައިސާގެ އަދަދާއި ދިވެހި ބަހުން ލިޔެފައިވާ ފައިސާގެ އަދަދު ތަފާތުވާނަމަ، ރަގަޅު އަދަދުކަމުގައި ބަލާނީ ދިވެހި ބަހުން ލިޔެފައިވާ ފައިސާ އަދަދެވެ. |
| 1. **ބީލަންތައް ޗެކްކުރުމާއި ބީލަންތަކުގެ ރެންޕޮންސިވްނަސް ކަނޑައެޅުއް**
 |  | ބީލަންތައް އިވެލުއޭޓްކުރުމުގެ ކުރިން ތިރީގައިވިމާ ކަންކަން ފުރިހަމަވޭތޯ ބެލޭނެއެވެ. |
|  | 22.1.1 ބީލަމަށް ޝަރުތު ފުރިހަމަވާ ފަރާތެއްކަން. |
|  | 22.1.2 ހުށަހަޅަންޖެހޭ ލިޔުންތައް ހުށަހަޅާފައިވާ ފަރާތެއްކަން  |
|  | 22.1.3 ބީލަމުގައިވާ އުސޫލްތަކަށްބަލައި އެކަށީގެންވާ ބިޑެއްތޯ ކަނޑައެޅުން (ރެންޕޮންސިވްނަސް) |
| 1. **ބީލަންތައް އިވޭލުއޭޓް ކުރުން**
 |  | ހުށަހަޅާ ބީލަންތަކުގެ ތެރެއިން އިވެލުއޭޓް ކުރެވޭނީ 22.1 ގައިވާ ކަންކަން ފުރިހަމަވާ ބީލަންތަކެވެ. |
| 1. **ބީލަން ހަވާލުކުރާނެ ފަރާތް ކަނޑައެޅުން**
 |  | ބީލަން ހަވާލުކުރާނެ ފަރާތެއް ކަނޑައަޅާނީ، ބީލަން ވަޒަންކުރުމަށް ބޭނުން ކުރާނެ މިންގަނޑަށް ބަލައިގެން އެންމެގިނަ މާކްސްލިބޭ ފަރާތަކަށެވެ. އަދި ބީލަން ހަވާލުކުރުމުގައި ދައުލަތުގެ އޮފީސްތަކުން ކުރިޔަސްގެންދާ ބީލަންތަކުގައި ވަކިވަކި ފަރާތްތަކާއި ދާއިރާތަކަށް އިސްކަންދިނުމުގައި ޢަމަލުކުރާނެ ގޮތުގެ އުސޫލު (އުސޫލު ނަންބަރު: 2022/G-23) އަށް އަމަލުކުރެވޭނެއެވެ.  |
| 1. **ބީލަންތަން ކެންސަލްކުރުން**
 |  | ބީލަންތައް ބަލައިގަތުމަށްފަހު ފުރިހަމަނުވާ ބީލަންތައް ބާތިލްކުރުމުގެ އިޚްތިޔާރު ވެރިފަރާތަށް ލިބިގެންވެއެވެ. އަދި ބީލަންތައް ބަލައިގަތުމަށްފަހު ހުށަހަޅާފައިވާ އަގުތަކަކީ އެކަށީގެންނުވާ އަގުތަކެއްނަމަ ނުވަތަ އެކަށީގެންވާ އަދަދަކަށް ބީލަން ހުށަހަޅާފައިނުވާނަމަ ބީލަންތައް ކެންސަލްކުރުމުގެ އިޚްތިޔާރު މަސައްކަތުގެ ވެރިފަރާތަށް ލިބިގެންވެއެވެ. |
| 1. **ބީލަން ކާމިޔާބުކުރާ ފަރާތް ހޮވައި، އެކަން އެންގުން**
 |  | ބީލަން ކާމިޔާބުވި ފަރާތަށާއި، ކާމިޔާބުނުވި ފަރާތްތަކަށް ލިޔުމުން އަންގާނެއެވެ. |
| 1. **އެއްބަސްވުމުގައި ސޮއި ކުރުން**
 |  | ބީލަން ކާމިޔާބުކުރިފަރާތަށް އެކަމުގެ ލިޔުން ފޮނުވާތާ ގިނަވެގެން ބަންދުނޫން 05 (ފަހެއް) ދުވަހުގެ ތެރޭގައި ބީލަން ކާމިޔާބުކުރި ފަރާތާއި ދެމެދު މަސައްކަތުގެ އެއްބަސްވުމުގައި ސޮއި ކުރަންވާނެއެވެ. |
|  |  | 27.1 ގައި ބަޔާންކޮށްފައިވާ ގޮތުގެމަތިން އެ މުއްދަތުގައި އެއްބަސްވުމުގައި ސޮއި ނުކުރައްވައިފިނަމަ، މިމަސައްކަތް ހަވާލުކުރުމަށް ނިންމާފައިވާ ނިންމުން ބާތިލްކުރެވޭނެއެވެ. |
|  |  | އެއްބަސްވުމުގައި ސޮއިކުރުމަށްފަހު މަސައްކަތް ދޫކޮށްލައިފިނަމަ ނުވަތަ އެއްބަސްވުމުގައި ސޮއިކުރުމަށްފަހު މަސައްކަތްފުރިހަމަ ނުކޮށް މަސައްކަތް ދޫކޮށްލައިފިނަމަ ދައުލަތުގެ މާލިއްޔަތުގެ ޤަވާއިދުގެ 17.19 ގައި ބަޔާންކޮށްފައިވާ ގޮތުގެމަތިން ފިޔަވަޅުއެޅޭނެއެވެ. |
| **(ޅ) ހުށަހަޅަންޖެހޭ ސެކިޔުރިޓީތައް** |
| 1. **ބިޑް ސެކިޔުރިޓީ**
 |  | ބީލަމަށް ޝީޓްގައި ބަޔާން ކޮށްފައިވާ އަދަދު ބިޑް ސެކިއުރިޓީ ހުށަހަޅަންވާނެއެވެ |
|  |  | ބިޑް ސެކިއުރިޓީގެ މުއްދަތަކީ ބިޑް ހުޅުވާ ދުވަހުން ފެށިގެން 60 (ފަސްދޮޅަސް) ދުވަހެވެ. |
|  |  | ބިޑް ސެކިއުރިޓީގެ ގޮތުގައި ހުށަހަޅަންޖެހޭނީ ސަރުކާރުން ގަބޫލުކުރެވޭ ބޭންކަކުން ނުވަތަ ދިވެހިރާއްޖޭގައި ގާއިމްކުރެވިފައިވާ ފައިނޭންޝަލް އިންސްޓިޓިއުޓަޝަނަކުން މި ޕްރޮޖެކްޓަކަށް ދޫކޮށްފައިވާ ސެކިއުރިޓީ ނުވަތަ ގެރެންޓީއެކެވެ. ބިޑް ސެކިއުރިޓީ އޮންނަންވާނެ ގޮތުގެ ނަމޫނާއެއް ޖަދުވަލު 7 ގައި ވާނެއެވެ. |
|  |  | ބީލަން ކާމިޔާބު ކުރާ ފަރާތަށް އެކަން އަންގާ ތާރީޚުން ފެށިގެން ރަސްމީ ބަންދު ނޫން 7 (ހަތެއް) ދުވަހުގެ ތެރޭގައި ބީލަން ކާމިޔާބު ނުވާ ފަރާތްތަކުގެ ބިޑް ސެކިއުރިޓީ އެފަރާތްތަކަށް ރައްދު ކުރެވޭނެ އެވެ. |
|  |  | ބީލަން ހުޅުވުމަށްފަހު ބީލަން ހުށަހެޅި ފަރާތަކުން ބީލަމުން ވަކިވެއްޖެނަމަ ނުވަތަ ބީލަން ކާމިޔާބުކުރާ ފަރާތަށް ބީލަން ކާމިޔާބުވިކަމުގެ ލިޔުން ލިބުމަށްފަހު ބީލަން ކެންސަލް ކޮށްފިނަމަ އެފަރާތުން ހުށަހަޅާފައިވާ ބިޑް ސެކިއުރިޓީ ދައުލަތަށް ނެގޭނެއެވެ.  |
| 1. **އެޑްވާންސް ފައިސާ އަދި އެޑްވާންސް ފައިސާގެ ގެރެންޓީ**
 |  | އެޑްވާންސް ފައިސާ ދިނުމަށް ހަމަޖެހިފައިވާ ޕްރޮޖެކްޓެއްނަމަ، އެޑްވާންސް ފައިސާއަށްއެދި އެދި ކޮންޓްރެކްޓަރު ހުށަހެޅުމުން ދައުލަތުގެ މާލިއްޔަތުގެ ގަވާއިދާ އެއްގޮތަށް އެޑްވާންސް ފައިސާ ދޫކުރެވިދާނެއެވެ. |
|  | އެޑްވާންސް ފައިސާ ދޫކުރެވޭނީ ޕްރޮކިއުމަންޓްގެ ޖުމްލަ އަގު 250,000/- (ދެލައްކަ ފަންސާސް ހާސް) ދިވެހި ރުފިޔާއަށްވުރެ ބޮޑުވާނަމައެވެ. |
|  | އެޑްވާންސް ފައިސާ ހޯދުމަށްއެދި ހުށަހަޅާނަމަ، މަސައްކަތް ހަވާލުވާތާ 45 (ސާޅީސް ފަހެއް) ދުވަހުގެ ތެރޭގައި އެޑްވާންސް ފައިސާއަށް އެދި ހުށަހަޅަންވާނެއެވެ. |
|  |  | އެޑްވާންސް ފައިސާ ހޯދުމަށް ހުށަހަޅާނަމަ އެޑްވާންސް ޕޭމަންޓް ގެރެންޓީގެ ގޮތުގައި ސަރުކާރުން ގަބޫލުކުރެވޭ ބޭންކަކުން ނުވަތަ ދިވެހިރާއްޖޭގައި ގާއިމްކުރެވިފައިވާ ފައިނޭންޝަލް އިންސްޓިޓިއުޝަނަކުން މި ޕްރޮޖެކްޓަކަށް ދޫކޮށްފައިވާ ސެކިއުރިޓީ ނުވަތަ ގެރެންޓީއެއް ހުށަހަޅަންވާނެއެވެ. އެޑްވާންސް ޕޭމަންޓް ސެކިއުރިޓީ އޮންނަންވާނެ ގޮތުގެ ނަމޫނާއެއް ޖަދުވަލު 9 ގައި ވާނެއެވެ. |
|  |  | އެޑްވާންސް ފައިސާގެ ގޮތުގައި ދޫކުރެވޭނީ މަސައްކަތުގެ ޖުމްލަ އަގުގެ 15% (ފަނަރަ އިންސައްތަ) އަށްވުރެ ބޮޑުނުވާ އަދަދެކެވެ. އަދި އެޑްވާންސްގެ ގޮތުގައި ދެވޭ ފައިސާ މަސައްކަތް ކުރަމުންދާއިރު ނުވަތަ ޚިދުމަތް ހޯދަމުންދާއިރު ހުށަހަޅާ ބިލްތަކުން، ކޮންޓްރެކްޓްގެ ޖުމްލަ އަގުގެ ނިސްބަތުން އުނިކުރެވޭނެއެވެ. |
| 1. **ޕާރފޯމަންސް ގެރެންޓީ**
 |  | ބީލަމަށް ހުށަހަޅާ އަގަކީ 500,000/- ރުފިޔާއަށްވުރެ މަތީގެ އަގެއްނަމަ ބީލަން ކާމިޔާބުކުރި ފަރާތުން ސަރުކާރު ގަބޫލުކުރާ ބޭންކަކުން ނުވަތަ ދިވެހިރާއްޖޭގައި ގާއިމްކުރެވިފައިވާ ފައިނޭންޝަލް އިންސްޓިޓިއުޝަނަކުން މި ޕްރޮޖެކްޓަށް ދޫކޮށްފައިވާ ސެކިއުރިޓީ ނުވަތަ ގެރެންޓީއެއް ޕާރފޯމަންސް ގެރެންޓީގެ ގޮތުގައި ހުށަހަޅަންވާނެއެވެ. |
|  |  | ޕާރފޯމަންސް ގެރެންޓީ ބެހެއްޓުމަށް ބީލަން ކާމިޔާބުކުރި ފަރާތަށް ދެވޭ މުއްދަތުގައި ޕާރފޯމަންސް ގެރެންޓީ ނުބަހައްޓައިފިނަމަ، މިމަސައްކަތް ހަވާލުކުރުމަށް ނިންމާފައިވާ ނިންމުން ބާތިލްކުރުމަށްފަހު، އެފަރާތުން ހުށަހަޅާފައިވާ ބިޑް ސެކިއުރިޓީ ދައުލަތަށް ނެގޭނެއެވެ. |
|  |  | ޕާރފޯމަންސް ގެރެންޓީގެ ގޮތުގައި ހުށަހަޅަންވާނީ ސަރުކާރު ގަބޫލުކުރާ ބޭންކަކުން ނުވަތަ ދިވެހިރާއްޖޭގައި ގާއިމްކުރެވިފައިވާ ފައިނޭންޝަލް އިންސްޓިޓިއުޓަޝަނަކުން މި ޕްރޮޖެކްޓަށް ދޫކޮށްފައިވާ ސެކިއުރިޓީ ނުވަތަ ގެރެންޓީއެކެވެ. ޕާރފޯމަންސް ގެރެންޓީ އޮންނަންވާނެ ގޮތުގެ ނަމޫނާއެއް ޖަދުވަލު 8 ގައި ވާނެއެވެ. |
| 1. **މައްސަލަ ހުށަހެޅުމާއި މައްސަލަ ބެލުން**
 |  | ދައުލަތުގެ މާލިއްޔަތުގެ ގަވާއިދުގެ 17.09 ގައި ބަޔާންކޮށްފައިވާ ފަދައިން ބީލަމެއްގައި ގަވާއިދާ ޚިލާފަށް ކުރާ ކަންތައްތައް ބެލުމަށް މައްސަލަ ހުށަހެޅުމާއި، ހުށަހެޅޭ މައްސަލަތައް ބެލުމުގައި ޢަމަލުކުރެވޭނީ، ދައުލަތުގެ މާލިއްޔަތާބެހޭ ސަރކިއުލަރ ނަންބަރު 13-K/CIR/2018/01 ގެ ޖަދުވަލު 17 ގައިވާ "ބީލަމަކާ ގުޅިގެން މައްސަލަ ހުށަހެޅުމާއި، ހުށަހެޅޭ މައްސަލަތައް ބެލުމުގައި ޢަމަލުކުރާނެގޮތުގެ އުޞޫލު" އާ އެއްގޮތަށެވެ. |
|  |  | ދައުލަތުގެ މާލިއްޔަތުގެ ގަވާއިދުގެ 17.09 ގައި ބަޔާންކޮށްފައިވާ ފަދައިން ބީލަމެއްގައި ގަވާއިދާ ޚިލާފަށް ކުރާ ކަންތައްތައް ބެލުމަށް ހުށަހަޅަންވާނީ ދައުލަތުގެ މާލިއްޔަތާބެހޭ ސަރކިއުލަރ ނަންބަރު 13-K/CIR/2018/01 ގެ ޖަދުވަލު 18 ގައިވާ "ބީލަން އިޢުލާންކުރި އޮފީހުގެ ޕްރޮކިއުމަންޓް އޮފިސަރަށް ބީލަންވެރިޔާ މައްސަލަ ހުށަހަޅާ ފޯމް-ފުރަތަމަ މަރުހަލާ" PR-14 ފޯމުންނެވެ. |
|  |  | ދައުލަތުގެ މާލިއްޔަތުގެ ގަވާއިދުގެ 17.09 ގައި ބަޔާންކޮށްފައިވާ ފަދައިން ބީލަމެއްގައި ގަވާއިދާ ޚިލާފަށް ކުރާ ކަންތައްތައް ބެލުމަށް ހުށަހެޅުމުން، މައްސަލަ ހުށަހަޅާ ތާރީޚުން ފެށިގެން ސަރުކާރު ބަންދު ނޫން 7 (ހަތެއް) ދުވަހުގެ ތެރޭގައި، މައްސަލަ ނިންމައި، މައްސަލަ ނިންމިގޮތް ލިޔުމަކުން މައްސަލަ ހުށަހެޅި ފަރާތަށް، ދައުލަތުގެ މާލިއްޔަތާބެހޭ ސަރކިއުލަރ ނަންބަރު 13-K/CIR/2018/01 ގެ ޖަދުވަލު 19 ގައިވާ "ބީލަމުގެ މައްސަލައާއި ގުޅިގެން ޕްރޮކިއުމަންޓް އޮފިސަރުދޭ ޖަވާބު" PR-14 ފޯމުން ޖަވާބު ތައްޔާރުކޮށް އަންގާނެއެވެ. |
|  |  | ދައުލަތުގެ މާލިއްޔަތުގެ ގަވާއިދުގެ 17.09 ގައި ބަޔާންކޮށްފައިވާ ފަދައިން ބީލަމެއްގައި ގަވާއިދާ ޚިލާފަށް ކުރާ ކަންތައްތައް ބެލުމަށް ހުށަހެޅުމުން، ޕްރޮކިއުމަންޓް އޮފިސަރުދޭ ޖަވާބާމެދު ހިތްހަމަ ނުޖެހޭނަމަ އެކަން ބަޔާންކޮށް މައްސަލަ އަލުން ބެލުމަށް މިނިސްޓްރީ އޮފް އެޑިޔުކޭޝަންގެ އޮޑިޓް އެންޑް ކޮމްޕްލަޔަންސް ސެކްޝަނަށް ހުށަހެޅިދާނެއެވެ. |
| 1. **މައްސަލަ އަލުން ބެލުމަށް މުސްތަޤިއްލު ރިވިއު ކޮމިޓީއަށް ހުށަހެޅުން**
 |  | ދައުލަތުގެ މާލިއްޔަތުގެ ގަވާއިދުގެ ބާބު 17.11 ގައި ބަޔާންކޮށްފައިވާ ފަދައިން ބީލަމެއްގައި ދިމާވާ މައްސަލައަކާއި ގުޅިގެން އިދާރީކަންކަން އަލުން ބެލުމަށް "މުސްތަޤިއްލު ރިވިޔު ކޮމެޓީ" އަށް ހުށަހެޅުމުގައި، ދައުލަތުގެ މާލިއްޔަތާބެހޭ ސަރކިއުލަރ ނަންބަރު 13-K/CIR/2018/01 ގެ ޖަދުވަލު 21 ގައިވާ "ބީލަންވެރިޔާ ބީލަމުގެ މައްސަލަ އަލުން ބަލައިދިނުމަށް އެދި "ބީލަމުގެ މައްސަލަ އަލުން ބަލާ މުސްތަޤިއްލު ރިވިޢު ކޮމެޓީއަށް މައްސަލަ ހުށަހަޅާ ފޯމު" – އެޕީލް މަރުހަލާ" PR-16 ފޯމުން ހުށަހަޅިދާނެއެވެ. |

|  |
| --- |
| **ސެކްޝަން - 3** |
| **އެއްބަސްވުމުގެ އާންމު މާއްދާތައް** **އަދި ހާއްސަ މާއްދާތައް** |
| 1. **މާނަކުރުން**
 |  | "މަސައްކަތުގެ ވެރިފަރާތް" ކަމަށް ބުނެފައި އެވަނީ، އެ މަސައްކަތެއް ކުރުމަށް ބޭނުންވާ މިނިސްޓްރީގެ ދާއިރާގެ ތަނަކަށެވެ.  |
|  |  | "މަސައްކަތް ހަވާލުވާ ފަރާތް" ކަމަށް ބުނެފައި އެވަނީ، އެ މަސައްކަތެއް ކޮށްދިނުމަށް އެދި ބީލަން ހުށަހަޅާ ފަރާތަށެވެ. |
|  |  | "މަސައްކަތް" ކަމަށް ބުނެފައިއެވަނީ ބީލަން ޝީޓްގައި ބަޔާންކޮށްފައިވާ ޚިދުމަތް ނުވަތަ މަސައްކަތަކެވެ. |
|  |  | "މަސައްކަތުގެ އަގު" ކަމަށް ބުނެފައިއެވަނީ އެއްބަސްވުމާއި އެއްގޮތަށް މަސައްކަތް ފުރިހަމަކުރުމުން މަސައްކަތް ހަވާލުވާ ފަރާތަށް ދައްކާ ފައިސާއަށެވެ.  |
|  |  | "އެއްބަސްވުން" ކަމަށް ބުނެފައި އެވަނީ، މަސައްކަތުގެ ވެރިފަރާތާއި، މަސައްކަތްކުރުމަށް ހަވާލުވާ ފަރާތާ ދެމެދު މަސައްކަތްކުރުމާބެހޭ ގޮތުން ވެވޭ އެއްބަސްވުމަށެވެ. |
| 1. **ލިޔެކިޔުން ބަދަލުކުރުން**
 |  | މި އެއްބަސްވުމުގައި ޝާމިލުވާ ފަރާތްތަކުން މިއެއްބަސްވުމާއި ގުޅިގެން އެއް ފަރާތުން އަނެއް ފަރާތަށް އަންގަންޖެހޭ އެންމެހައި އެންގުންތައް އާއްމުގޮތެއްގައި އަންގާނީ ދިވެހި ބަހުން، ލިޔުމުންނެވެ. |
|  |  | އެއްފަރާތުން އަނެއް ފަރާތަށް ފޮނުވާ ލިޔުން ރައްދުކުރާނީ އަތުން އަތަށް ނުވަތަ ރަޖިސްޓްރީ ފޯސްޓުން، ނުވަތަ ކަނޑައެޅިފައިވާއީމެއިލަށް، ބީލަމުގައި ބަޔާން ކޮށްފައިވާ އެޑްރެހަށެވެ. |
|  |  | މިއެއްބަސްވުމުގައިވާ އެޑްރެސް ބަދަލުކުރާން ބޭނުންވާނަމަ، ބަދަލު ކުރާން ބޭނުންވާ ފަރާތުން އަނެއް ފަރާތަށް ލިޔުމުން އަންގަންވާނެއެވެ. |
| 1. **ތިންވަނަ ފަރާތަކާއި މަސައްކަތް ހަވާލުކުރުން**
 |  | މިއެއްބަސްވުމުގެ ދަށުންކުރެވޭ މަސައްކަތުގެ އެއްވެސްބައެއް އެހެންފަރާތަކާއި ޙަވާލުކޮށްގެން ކުރަން ބޭނުންވާނަމަ އެކަން ބަޔާންކޮށް މަސައްކަތް ޙަވާލުވާ ފަރާތުން، ވެރިފަރާތަށް ލިޔުމުން ހުށަހަޅާ ހުއްދަހޯދަށްވާނެއެވެ. |
|  | 35.1 ގައިވާ ގޮތުގެމަތިން އެހެން ފަރާތަކާ މަސައްކަތުގެ އެއްވެސްބައެއް ހަވާލުކުރިކަމުގައިވިޔަސް މަސައްކަތް ޙަވާލުވާ ފަރާތުން މިއެއްބަސްވުމުގައިވާގޮތުގެމަތިން ފުރިހަމައަށް ޒިންމާ އުފުލަން ވާނެއެވެ. |
| 1. **ތަކެއްޗާއި ޚިދުމަތާއި ހަވާލުވުން**
 |  | ތަކެތި ގުދަނަށް ގެނައުމުގެ 03 (ތިނެއް) ދުވަސް ކުރިން ތަކެތި ގުދަނަށް ގެނެވޭނެ ތާރީޚާއި ގަޑި މަސައްކަތް ވިލަރެސްކުރާ ފަރާތަށް އަންގަންވާނެއެވެ.  |
|  | ތަކެތި ގުދަނަށް ގެނައުމުން މަސައްކަތް ވިލަރެސްކުރާ ފަރާތުން (ގުދަނުން) ޙަވާލުވާނީ ތަކެތީގެ އަދަދާއެވެ. |
|  |  | އެއްބަސްވުމުގައިވާ ގޮތަށް ތަކެތި/ޚިދުމަތް ލިބިފައިވޭތޯ ބަލާނީ ގުދަނަށް ޙަވާލުވުމަށްފަހު އިވެލުއޭޝަން ކޮމެޓީންނެވެ. ކޮލިޓީ ބެލުމަށްފަހު ސްޕެސިފިކޭޝަނާއި އެއްގޮތަށް މަސައްކަތް ނިންމާފައިވާކަމަށް ވާނަމަ އެގްރީމަންޓާ އެއްގޮތަށް ތަކެތި/ޚިދުމަތް ލިބުނުކަމަށްބެލޭނެއެވެ. އަދި އެއްބަސްވުމާ ޚިލާފަށް ފޯރުކޮށްދީފައިވާ ޚިދުމަތް/ތަކެތި އަނބުރާ ފޮނުވާލެވޭނެއެވެ. |
| 1. **އެއްބަސްވުމުގެ މުއްދަތު**
 |  | އެއްބަސްވުމުގައި ބަޔާންކޮށްފައިވާ މުއްދަތުގެ ތެރޭގައި ތަކެތި/ޚިދުމަތް ފޯރުކޮށްދޭންވާނެއެވެ |
|  | މަސައްކަތް ހަވާލުވިފަރާތުގެ ބާރުނުފޯރާ ކަމެއް ނުވަތަ ޤުދުރަތީ ޙާދިސާއެއް/ކާރިޘާއެއް ނުވަތަ މެނިފެކްޗަރިންއާއި ގުޅޭކަމެއް ކުރިމަތިވެއްޖެނަމަ މުއްދަތު އިތުރުކުރުމަށްޓަކައި އެޙާދިސާއެއް/ކާރިޘާއެއް ނުވަތަ އެކަމެއް ދިމާވިކަން އެގޭފަދަ (ރަސްމީ ނުވަތަ ކަމާގުޅޭ ފަރާތްތަކުގެ) ލިޔުންތަކާއެކު މަސައްކަތް ނިންމަންޖެހޭ މުއްދަތު ހަމަވުމުގެ ކުރިން މަސައްކަތުގެ ވެރިފަރާތަށް ހުށަހަޅަންވާނެއެވެ.  |
|  |  | އެއްވެސް ސަބަބަކާއި ހުރެ މުއްދަތު އިތުރުކޮށްދިނުމަށް ހުށަހެޅިނަމަވެސް މުއްދަތު އިތުރުކޮށްދޭނީ "މުއްދަތު އިތުރުކޮށްދިނުމުގެ އުޞޫލު" ގައި ބަޔާންކޮށްފައިވާ ގޮތުގެމަތިން ބިޑް ކޮމެޓީއަށް ހުށަހަޅައިގެންނެވެ. |
| 1. **ޖުރިމަނާ ކުރުމާއި އެގްރީމަންޓް ބާތިލް ކުރުން**
 |  | އެއްބަސްވުމުގައިވާ މުއްދަތަށް މަސައްކަތް ނުނިމޭނަމަ ދައުލަތުގެ މާލިއްޔަތުގެ ޤަވާއިދުގެ 10.71 ވަނަ މާއްދާއާ އެއްގޮތްވާ ގޮތުގެމަތިން ލިކުއިޑޭޓަޑް ޑެމޭޖަސް ކެނޑޭނެއެވެ.  |
|  | ޖުމްލަ އަގު 2,500,000/-ރުފިޔާއަށްވުރެ ދަށުގެ ބީލަމެއްނަމަ ފައިސާ ކަނޑާނީ، ޖުމުލަ އަގު 0.005 (ޕޮއިންޓް ސުމެއް ސުމެއް ފަހެއް) އާ ގުނަކުރުމުން ޖެހޭ އަދަދާ މުއްދަތަށްވުރެ އިތުރުވާ ދުވަސްތަކުގެ އަދަދާ ގުނަކުރުމުން ޖެހޭ އަދަދެކެވެ.ލިކުއިޑޭޓެޑް ޑެމޭޖަސް = CP\*0.005\*LDCP (ކޮންޓްކެޓް ޕްރައިސް): ކޮންޓްރެކްޓްގެ ޖުމްލަ އަގުLD (ލޭޓް ޑިއުރޭޝަން): ކޮންޓްރެކްޓްގެ މުއްދަތަށްވުރެ އިތުރުވާ ދުވަސްތައް |
|  |  | ޖުމްލަ އަގު 2,500,000/-ރުފިޔާއަށްވުރެ މަތީގެ ބީލަމެއްނަމަ ފައިސާ ކަނޑާނީ، ޖުމުލަ އަގު 0.0025 (ޕޮއިންޓް ސުމެއް ސުމެއް ދޭއް ފަހެއް) އާ ގުނަކުރުމުން ޖެހޭ އަދަދާ މުއްދަތަށްވުރެ އިތުރުވާ ދުވަސްތަކުގެ އަދަދާ ގުނަކުރުމުން ޖެހޭ އަދަދެކެވެ.ލިކުއިޑޭޓެޑް ޑެމޭޖަސް = CP\*0.025\*LDCP (ކޮންޓްކެޓް ޕްރައިސް): ކޮންޓްރެކްޓްގެ ޖުމްލަ އަގުLD (ލޭޓް ޑިއުރޭޝަން): ކޮންޓްރެކްޓްގެ މުއްދަތަށްވުރެ އިތުރުވާ ދުވަސްތައް |
|  |  | މަސައްކަތް ނުނިމި ލަސްވާ މުއްދަތަށް މަސައްކަތް ޙަވާލުވި ފަރާތުން ފައިސާ ދޭންޖެހިއްޖެނަމަ، މަސައްކަތް ޙަވާލުވި ފަރާތުން ހުށަހަޅާ ބިލަށް ފައިސާ ދޫކުރެވޭނީ މަސައްކަތް ނުނިމި ލަސްވީ މުއްދަތަށްވާ ފައިސާ ބިލްގައިވާ އަދަދުން ކެނޑުމަށްފަހު ބާކީ ފައިސާއެވެ. |
|  |  | މަސައްކަތުގެ ޖުމްލަ އަގުގެ %15 އިންސައްތަ އަށްވުރެ ލިކުއިޑޭޓަޑް ޑެމޭޖަސް ބޮޑުވެއްޖެނަމަ އެއްބަސްވުން ބާތިލްކުރެވޭނެއެވެ. |
| 1. **އެގްރީމަންޓް ބާތިލްކުރުން**
 |  | އެއްބަސްވުމުގައި ބަޔާންކޮށްފައިވާގޮތަށް މަސައްކަތް ކުރިޔަށް ނުދާކަމަށް ފާހަގަ ކުރެވިއްޖެނަމަ އެއްބަސްވުންއެއްކޮށް ނުވަތަ އެއްބަސްވުމުގެ ބައެއް ބާތިލްކުރުމުގެ ފުރިހަމަ އިޚްތިޔާރު މަސައްކަތުގެ ވެރިފަރާތަށް ލިބިގެންވެއެވެ. |
|  |  | އެއްވެސް ސަބަބަކާހުރެ އެއްބަސްވުން ބާތިލްކޮށްފިނަމަ ބަންދުނޫން 3 ދުވަހުގެ ތެރޭގައި، އެހާތަނަށް ނިމިފައިވާ މަސައްކަތާއި، ނުނިމިހުރި މަސައްކަތުގެ ތަފްސީލް އަގާއެކު ލިޔެ، ދެފަރާތުން އެލިޔުމުގައި ސޮއިކުރަން ވާނެއެވެ. އަދި މަސައްކަތް ހިނގާ ސައިތްގައި ހުންނަ ކޮންޓްރެކްޓަރ ގެ ހުރިހާ ތަކެތީގެ ލިސްޓް ނަގައި އެތަކެތި ބަނދުނޫން 3 ދުވަހުގެ ތެރޭގައި ގެންދަންވާނެއެވެ. މި މުއްދަތުގެ ފަހުން މިއިން އެއްޗަކަށް ދިމާވާ އެއްވެސް މައްސަލައަކަށް ޒިންމާއެއް ނުވެވޭނެއެވެ. |
| 1. **އެހެނިހެން ކަންކަން**
 |  | މި އެއްބަސްވުމުގައި ދެފަރާތުން ސޮއިކުރުމަށްފަހު ސަރުކާރުގެ އެއްވެސް ޤާނޫނެއް ނުވަތަ ގަވާއިދަކާ މި އެއްބަސްވުމާއި ތަޢާރުޟު ވާކަން އެނގިއްޖެނަމަ ނުވަތަ އެފަދަ ޤާނޫނެއް ނުވަތަ ގަވާއިދެއް ހެދިއްޖެނަމަ އެކަމެއްގެ ސަބަބުން މުޅި މިއެއްބަސްވުން ބާޠިލެއް ނުވާނެއެވެ. އެފަދަ މާއްދާއެއް މި އެއްބަސްވުމުގައި ހިމެނިފައިވާނަމަ އެ މާއްދާއެއް އިސްލާހްކޮށްގެން ނަމަވެސް މި އެއްބަސްވުން އުވާނުލައި ދެމެހެއްޓުމަށް ދެފަރާތުންވެސް އެއްބަސްވެ ޤަބޫލުކުރަމެވެ. |
| 1. **ޓެކްސް އަދި އެހެނިހެން ފީތައް**
 |  | މިމަސައްކަތާއި ގުޅިގެން ދައްކަންޖެހޭ ޓެކްސްތަކާއި، ކަސްޓަމްސް ޑިޔުޓީތަކާއި، އިމްޕޯޓް ލައިސަންސް ފީތައް އަދި އެހެނިހެއް ފީއެއް ދައްކަންޖެހިއްޖެނަމަ ފީއެއް ދައްކާނީ މަސައްކަތް ހަވާލުވި ފަރާތުންނެވެ. |
| 1. **އެއްބަސްވުމަށް ބަދަލުގެނައުން**
 |  | މި އެއްބަސްވުމުގައިވާ އެއްވެސް މާއްދާއަކަށް ބަދަލެއް ގެނެވޭނީ ދެފަރާތުގެ މެދުގައި ސޮއިކުރެވޭ އެއްބަސްވުމަކުންނެވެ. |
| 1. **އެއްބަސްވުމަށް ހިނގާނެ ޤާނޫނު**
 |  | މި އެއްބަސްވުން ހިންގާނީ، އަދި ތަންފީޛު ކުރާނީ ދިވެހިރާއްޖޭގެ ޤާނޫނުތަކާއި ޤަވާއިދުތަކާއި އެއްގޮތަށެވެ. |
| 1. **ދެބަސްވުން**
 |  | މިއެއްބަސްވުމާއިމެދު އުފެދޭ ދެބަސްވުން ދެފަރާތުގެ މެދުގައި ވާހަކަ ދައްކައިގެން ހައްލުނުކުރެވިއްޖެނަމަ، ދިވެހިރާއްޖޭގެ ޝަރުޢީ ކޯޓަކަށް މައްސަލަ ހުށަހަޅައިގެން ނިންމާނީއެވެ.  |
|  |  | މިއެއްބަސްވުމުގައި ނެތްކަމެއް ދިމާވެއްޖެނަމަ އެކަމެއް ހައްލުކުރާނީވެސް ދެފަރާތުގެ މެދުގައި ވާހަކަ ދައްކައިގެންނެވެ. ހައްލުނުވެއްޖެނަމަ، ދިވެހިރާއްޖޭގެ ޝަރުޢީ ކޯޓަކަށް މައްސަލަ ހުށަހަޅައިގެން ނިންމާނީއެވެ. |

|  |
| --- |
| **ސެކްޝަން - 4** |
| **ޖަދުވަލުތައް** |
| **ޖަދުވަލު – 1** |
| **ބީލަން ހުށަހަޅާ ފަރާތުން ހުށަހަޅަންޖެހޭ ލިޔުންތައް އަދި ޗެކްލިސްޓް** |
|

|  |  |  |  |
| --- | --- | --- | --- |
| **#** | **ހުށަހަޅަންޖެހޭ ލިޔުންތައް** |  |  |
| **ބީލަން ހުށަހަޅާއިރު ތިރީގައިމިވާ މަޢުލޫމާތު އަދި ލިޔުމެއް އަދި ލިޔުންތައް މަދު ނުވަތަ ނެތްނަމަ ޑިސްކޮލިފައި ކުރެވޭނެއެވެ.**  |
| 1 | ބީލަން ހުށަހަޅާ ފޯމް (ޖަދުވަލު 2 ) |  |  |
| 2 | ކުންފުނި/ޕާޓްނަރޝިޕް/ ކޯޕަރޭޓިވް ސޮސައިޓީ/ އަމިއްލަ ފަރުދުންގެ ވިޔަފާރީގެ ރެޖިސްޓްރީގެ ކޮޕީ  |  |  |
| 3 | ހުށަހަޅާ އެސްޓިމޭޓް (ކޯޓޭޝަން / ބީ.އޯ.ކިޔު) (ބީލަމުގައި ހުށަހަޅަންޖެހޭނެ ކަމަށް ބަޔާންކުރާނަމަ) |  |  |
| 4 | ހުށަހަޅާ ފަރާތުގެ ޕްރޮފައިލް (ޖަދުވަލު 3) |  |  |
| 5 | ޖީއެސްޓީ ރެޖިސްޓްރޭޝަން ސެޓްފިކެޓް ކޮޕީ (ޖީ.އެސް.ޓީއަށް ރެޖިސްޓްރީކޮށްފައިވާނަމަ) |  |  |
| 6 | ބީލަމުގައި ސޮއިކުރުމުގެ ހުއްދަ ލިޔުން (ޕަވަރ އޮފް އެޓާރނީ) |  |  |
| 7 | 6.1 ވަނަ މާއްދާގައިވާ ބަޔާންކުރާ ލިޔުން ހުށަހަޅަންޖެހޭނަމަ އެލިޔުން. |  |  |
| 8 | ބިޑު ސެކިއުރިޓީ (ބިޑު ސެކިއުރިޓީ ހުށަހަޅަންޖެހޭ ޕްރޮޖެކްޓްތަކަށް) |  |  |
| 9 | ސްޕެސިފިކޭޝަން ފޯމް (ޖަދުވަލު - 10) (ބީލަމުގައި ހުށަހަޅަންޖެހޭނެ ކަމަށް ބަޔާންކުރާނަމަ) |  |  |
| 10 | ހުށަހަޅާ ޓެކްނިކަލް ޓީމްގެ މަޢުލޫމާތު، ސީ.ވީ،އެކްރެޑިޓެޑް ސެޓްފިކެޓްތައް (ޖަދުވަލު - 11) |  |  |
| **ބީލަން ހުށަހަޅާއިރު ތިރީގައިމިވާ މަޢުލޫމާތު އަދި ލިޔުމެއް އަދި ލިޔުންތައް މަދު ނުވަތަ ނެތްނަމަ މާރކްސް ނުލިބޭނެއެވެ.** |
| 11 | ޖަދުވަލު 4 "މާލީ ތަނަވަސްކަމާއި ބެހޭ މަޢުލޫމާތު" ފުރިހަމަކޮށް ހުށަހަޅާފައި |  |  |
| 12 | ޖަދުވަލު 4 "މާލީ ތަނަވަސްކަމާއި ބެހޭ މަޢުލޫމާތު" ގައި ބަޔާންކުރާ ލިޔުންތައް ހުށަހަޅާފައި |  |  |
| 13 | ޖަދުވަލު 5 "ފާއިތުވި 3 (ތިނެއް) އަހަރުގެ ތެރޭގައި ކޮށްފައިވާ ގުޅުންހުރި މަސައްކަތްތައް" ފުރިހަމަކޮށް ހުށަހަޅާފައި |  |  |
| 14 | ޖަދުވަލު 5 "ފާއިތުވި 3 (ތިނެއް) އަހަރުގެ ތެރޭގައި ކޮށްފައިވާ ގުޅުންހުރި މަސައްކަތްތައް" ބަޔާންކުރާ މަސައްކަތުގެ ތަޖްރިބާގެ ލިޔުންތައް ހުށަހަޅާފައި |  |  |
| **ބީލަން ހުށަހަޅާއިރު ތިރީގައިމިވާ ލިޔުންތައް ހިމެނޭނަމަ، ބީލަމާއެކު ހުށަހެޅުއްވުމަށް.** |
| 15 | އެންމެ ކުދި، ކުދި އަދި މެދުފަންތީގެ ވިޔަފާރިއެއްގޮތުގައި ރަޖިސްޓްރީކޮށްފައިވާނަމަ، ރަޖިސްޓްރީގެ ކޮޕީ. |  |  |
| **ބީލަން ހުށަހަޅާއިރު ތިރީގައިމިވާ އިރުޝާދާ އެއްގޮތަށް ބީލަން ހުށަހަޅާފައިނުވާނަމަ ބީލަން ކެންސަލް ކުރުމުގެ އިޙްތިޔާރު ބީލަމަށް ހުޅުވާލި ފަރާތަށް ލިބިގެންވެއެވެ.** |
| 16 | ހުށަހަޅަންޖެހޭ ލިޔުންތައް ހުރީ މިލިސްޓުގައި ވާ ތަރުތީބުން ތަރުތީބުކުރެވިފައި  |  |  |
| 17 | ޞަފްހާ ނަންބަރު ޖަހާފައި (ކިތައް ޞަފްޙާގެ ތެރެއިން ކިތައްވަނަ ޞަފްޙާކަން އެނގޭގޮތަށް) |  |  |
| 18 | ޞަފްހާތަކުގައި ހުރީ ސޮއިކޮށްފައި  |  |  |
| 19 | ބީލަމުގެ ގަނޑުތައް ހުރީ ވަކިނުވާނެހެން ބައިންޑްކޮށް / ހީރަސްޖަހާފައި |  |  |
| **އެއްބަސްވުމުގައި ސޮއިކުރުމުގެ ކުރިން ހުށަހަޅަންޖެހޭ ލިޔުންތައް** |
| 20 | މޯލްޑިވްސް އިންލަންޑް ރެވެނިއު އޮތޯރިޓީން ދޫކުރާ ޓެކްސް ކްލިއަރެންސް ރިޕޯޓްގެ ކޮޕީ (ދޫކުރިފަހުން 3 މަސް ހަމަނުވާ) |  |  |
| 21 | ގަވާއިދުން ޕެންޝަން ފައިސާ ދައްކާކަމުގެ ލިޔުމުގެ ކޮޕީ (އެންމެފަހުން ދެއްކި މަހުގެ އަދި މުވައްޒަފުން ނެތްނަމަ ނެތްކަމަށް ޕެންސަން އޮފީހުންދީފައިވާ ލިޔުން) (ދޫކުރިފަހުން 3 މަސް ހަމަނުވާ) |  |  |
|  |

 |
| **ޖަދުވަލު – 2** |
| **ބީލަން ހުށަހަޅާ ފޯމް** |
|

|  |
| --- |
| 1. **ބީލަން ހުށަހަޅާ ފަރާތުގެ މަޢުލޫމާތު**
 |
|  | ނަން | 1.1 |
|  | އެޑްރެސް | 1.2 |
| 1. **ބީލަން ހުށަހަޅާ ޕްރޮޖެކްޓްގެ މަޢުލޫމާތު**
 |
|  | ޕްރޮޖެކްޓްގެ ނަން | 2.1 |
|  | އިޢުލާން ނަންބަރު | 2.2 |
| 1. **ހުށަހަޅާ އަގާއި މުއްދަތު**
 |
|  | ހުށަހަޅާ އަގު  | 3.1 |
|  | ޖީ.އެސް.ޓީ  |  |
|  | ޖުމްލަ އަގު: |  |
|  | ޖުމްލަ އަގު )ތާނައިން ލިޔުމަށް( | 3.2 |
|  | މުއްދަތު (ބަންދުދުވަސްތައް ހިމަނައިގެން) | 3.3 |
| 1. **ބީލަން ހުށަހަޅާ ފަރާތުގެ އިގްރާރު**
 |
| މަތީގައިބަޔާންކޮށްފައިވާ މަސައްކަތް/ޚިދުމަތް ފޯރުކޮށްދިނުމަށް ދީފައިވާ މަޢުލޫމާތާއި، އެގްރީމަންޓްގެ މާއްދާތައް ރަނގަޅަށް ބެލުމަށް ފަހު، މަތީގައި ދެންނެވިފައިވާ އަގަށް މި މަސައްކަތް ނުވަތަ ޚިދުމަތް ދިނުމަށް އަޅުގަނޑު / އަޅުގަނޑުމެން ބީލަން ހުށަހަޅަމެވެ. | 4.1 |
| އަޅުގަނޑު/ އަޅުގަނޑުމެންނަށް މަސައްކަތް/ޚިދުމަތް ފޯރުކޮށްދިނުން ހަވާލުކުރަން ނިންމައިފިނަމަ، އެކަށީގެންވާ މުއްދަތެއްގެ ތެރޭގައި މަސައްކަތް ފެއްޓުމަށާއި، 3.3 ގައިވާ މުއްދަތުގައި މަސައްކަތް/ޚިދުމަތް ފޯރުކޮށްދިނުމަށް ހުށަހަޅަމެވެ. | 4.2 |
| މިބީލަން ހުށަހަޅާތާ 60 ދުވަސް ހަމަވަންދެން މިބީލަން ޤަބޫލުކޮށް، އެއާއި އެއްގޮތަށް ޢަމަލުކުރުމަށް އަޅުގަނޑު / އަޅުގަނޑުމެން އެއްބަސްވަމެވެ. މިމުއްދަތުގެ ތެރޭގައި އެއްބަސްވުމުގައި ސޮއިކުރުމަށް ވެރިފަރާތުން އެދިވަޑައި ގެންފިނަމަ، އެއްބަސްވުމުގައި ސޮއިކޮށް އެއްބަސްވުމާއި އެއްގޮތަށް މަސައްކަތް ކުރުމަށްވެސް އެއްބަސްވަމެވެ.  | 4.3 |
| 1. **ބީލަން ހުށަހަޅާ ފަރާތުން**
 |
| އޮފިޝަލް ސްޓޭމްޕްއޮފިޝަލް ސްޓޭމްޕް | އޮފިޝަލް ސްޓޭމްޕް | ސޮއި |
|  | ނަން |
|  | މަޤާމު |
|  | ތާރީޚް |

 |
| **ޖަދުވަލު – 3** |
| **ހުށަހަޅާ ފަރާތުގެ ޕްރޮފައިލް** |
|

|  |
| --- |
| 1. **ހުށަހަޅާ ފަރާތުގެ މަޢުލޫމާތު**
 |
|  | ނަން |  |
|  | ރަޖިސްޓްރީ ކުރެވިފައިވާ އެޑްރެސް |  |
|  | ވިޔަފާރި އެޑްރެސް |  |
|  | ރަޖިސްޓްރީ ނަންބަރު |  |
|  | ޓެކްސް ޕޭޔަރ އައިޑެންޓިފިކޭޝަން ނަންބަރު |  |
|  | ޖީ.އެސް.ޓީ ޓިން ނަންބަރު |  |
|  | ފޯނު ނަންބަރު |  |
|  | އީމެއިލް އެޑްރެސް |  |
| 1. **ހުށަހަޅާ ފަރާތުގެ ވެރިންގެ މަޢުލޫމާތު (ކުންފުންޏެއްނަމަ ހިއްސާދާރުންގެ މަޢުލޫމާތު، ޕާޓްނަރޝިޕެންނަމަ ޕާޓްނަރުންގެ މަޢުލޫމާތު، އަމިއްލަ ފަރުދުންގެ ވިޔަފާރިއެއްނަމަ ވެރިފަރާތުގެ މަޢުލޫމާތު)**
 |
| **މަޤާމު** | **ނަން** | **#** |
| މެޖޭނިންގ ޑިރެކްޓަރ |  |  |
| ޑިރެކްޓަރ |  |  |
| ޑިރެކްޓަރ |  |  |
|  |  |  |
| 1. **އާންމުކޮށްކުރާ މަސައްކަތްތައް (ހުއްދަދީފައިވާ)**
 |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |

 |

|  |
| --- |
| **ޖަދުވަލު – 4** |
| **މާލީ ތަނަވަސްކަމާއި ބެހޭ މަޢުލޫމާތު**  |
|

|  |
| --- |
| **ފާއިތުވި 3 އަހަރުގެ ރެވެނިއު** |
| **#** | **އަހަރު** | **ފައިސާގެ އަދަދު** |
| 1 | 2019 |  |
| 2 | 2020 |  |
| 3 | 2021 |  |
|  | **ޖުމްލަ** |  |
|  | **އެވްރެޖް** |  |
| **ފާއިތުވި 3 އަހަރުގެ ކަރަންޓް އެސެޓްސް** |
| **#** |  | **ފައިސާގެ އަދަދު** |
| 1 | 2019 |  |
| 2 | 2020 |  |
| 3 | 2021 |  |
|  | **ޖުމްލަ** |  |
|  | **އެވްރެޖް** |  |

 |

|  |
| --- |
| **ޖަދުވަލު – 5** |
| **ފާއިތުވި 36 (ތިރީސް ހައެއް) މަހުގެ ތެރޭގައި ކޮށްފައިވާ ގުޅުންހުރި މަސައްކަތްތައް (2022 އޮކްޓޯބަރު މަހުގެ ނިޔަލަށް)** |
|

|  |
| --- |
| **ބީލަން ހުށަހަޅާ ފަރާތުގެ ކޮށްފައިވާ ގުޅުންހުރި މަސައްކަތްތަކުގެ ތަފްސީލް** |
| **މަސައްކަތުގެ އަގު (ދިވެހި ރުފިޔާއިން)** | **މަސައްކަތްކުރި އަހަރު** | **މަސައްކަތުގެ ވެރިފަރާތް** | **މަސައްކަތުގެ ނަން** | **#** |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  | **ޖުމްލަ:** |

**ނޯޓް:** އިވެލުއޭޝަނަށް ނެގޭނީ ހުށަހަޅާއަގުގެ **20 އިންސައްތަ** ހަމަވާ މަސައްކަތްތަކެވެ |
| **ޖަދުވަލު – 6** |
| **ބީލަން އިވޭލުއޭޓް ކުރުމަށް ބޭނުން ކުރާނެ މިންގަނޑު** |
|

|  |  |  |
| --- | --- | --- |
| ދާއިރާ | ތަފްސީލް | އިވެލުއޭޓް ކުރާނެގޮތް |
| އަސާސީ ޝަރުތުތައް | އަސާސީ ޝަރުތުތައް ފުރިހަމާ ބީލަމެއްތޯ ޗެކްކުރުން | ހުށަހަޅާ ލިޔުންތައް | މަދުވެގެން ހުންނަންޖެހޭ ވަރު |
| ރިކުއަރމަންޓަށް | ޚިދުމަތް ފޯރުކޮށްދިނުމަށް ކަޑައަޅާފައިވާ ރިކުއަރމަންޓަށް ފެތޭގޮތަށް ހުށަހަޅާފައިވާ ބީލަމެއްތޯ ޗެކްކުރުން | ބީލަމާއެކު ހުށަހަޅާ ލިޔުންތައް | - |
| މާލީ ޤާބިލުކަން | ޖަދުވަލު 4 ފުރިހަމަކޮށް ހުށަހަޅާފައިވާ ފާއިތުވި 3 އަހަރުގެ އެވްރެޖް އާމްދަނީ ( މަދުވެގެން 2 މިލިއަން ރުފިޔާ) | އޮޑިޓް ކޮށްފައިވާ މާލީ ހިސާބު |  MVR 2 Million |
| ޖަދުވަލު 4 ފުރިހަމަކޮށް ހުށަހަޅާފައިވާ ފާއިތުވި 3 އަހަރުގެ އެވްރެޖް ކަރަންޓް އެސެޓްސް ( މަދުވެގެން 0.5 މިލިއަން)  | އޮޑިޓް ކޮށްފައިވާ މާލީ ހިސާބު |  MVR 0.5 Million |
| ތަޖުރިބާ | ޖަދުވަލު 5 ފުރިހަމަކޮށް ހުށަހަޅާފައިވާ ފާއިތުވި 36 މަހު ކޮށްފައިވާ ގުޅުންހުރި މަސައްކަތްތައް (މަސައްކަތްތަކުގެ ޖުމްލަ އަގު 2 މިލިއަން)  | މަސައްކަތް ނިންމިކަމުގެ ލިޔުންތައް |  MVR 2 Million |
| ނޯޓް: އަގާ މުއްދަތަށް ޕޮއިންޓް ދެވޭނީ މަތީގައިވާ ބައިތަކުން ފާސްވާ ބީލަންތަކަށެވެ. |
| ޕޮއިންޓްދެވޭނެދާއިރާ | **ޕޮއިންޓް ދެވޭނެ ގޮތުގެ ތަފްސީލް** |  | **ޕޮއިންޓްގެ އަދަދު** |
| އަގު | ހުށަހެޅި އެންމެ ހެޔޮ އަގު/ ހުށަހެޅި އަގު × 85  |  | **85** |
| މުއްދަތު | ހުށަހެޅި އެންމެ ކުރު މުއްދަތު/ ހުށަހެޅި މުއްދަތު × 15  |  | **15** |
| ޖުމްލަ  |  | **100** |

 |

|  |
| --- |
| **ޖަދުވަލު – 7** |
| **ބިޑް ސެކިއުރިޓީ** |
| Form of Bid Security (Bank Guarantee)Whereas, ………………………………………………..*[name of Bidder]* (hereinafter called “the Bidder”) has submitted his Bid for the Tender no……….issued by the Ministry of Education on ………………………………… …………..for Supplying/Purchasing of …………………………… …….*[name of Contract]* (hereinafter called “the Bid”).Know all people by these presents that We ………………………………………. *[name of Bank]* of ……… …………………… *[name of country]* having our registered office at ………………………………………………………………………………….. (hereinafter called “the Bank”) are bound unto …………………………….*[name of Purchaser]* (hereinafter called “the Purchaser”) in the sum of \*………………………………………….. for which payment well and truly to be made to the said Purchaser, the Bank binds itself, its successors, and assigns by these presents.Sealed with the Common Seal of the said Bank this ……..day of …………….20……………..The conditions of this obligation are: (1) If, after Bid opening, the Bidder withdraws his Bid during the period of Bid validity specified in the Form of Bid; or(2) If the Bidder having been notified of the acceptance of his Bid by the Purchaser during the period of Bid validity: (a) fails or refuses to execute the Form of Agreement in accordance with the Instructions to Bidders, if required; or (b) fails or refuses to furnish the Performance Security, in accordance with the Instruction to Bidders; or (c) does not accept the correction of the Bid Price pursuant to Clause 27,

|  |
| --- |
| \* The Bidder should insert the amount of the Guarantee in words and figures denominated in Maldivian Rufiyaa. This figure should be the same as shown in Clause 16.1 of the Instructions to Bidders. |

we undertake to pay to the Purchaser up to the above amount upon receipt of his first written demand, without the Purchaser’s having to substantiate his demand, provided that in his demand the Purchaser will note that the amount claimed by him is due to him owing to the occurrence of one or any of the three conditions, specifying the occurred condition or conditions.This Guarantee will remain in force up to and including the date ………………………. days after the deadline for submission of bids as such deadline is stated in the Instructions to Bidders or as it may be extended by the Purchaser, notice of which extension(s) to the Bank is hereby waived. Any demand in respect of this Guarantee should reach the Bank not later than the above date.Date…………………………… Signature of the Bank  Witness ……………………… Seal *[signature, name, and address]* |
| **ޖަދުވަލު – 8** |
| **ޕާރފޯމަންޓް ގެރެންޓީ** |
| Form of Performance Bank Guarantee (Unconditional)To: …………………………………………………………………………………………………. *[name &address of Purchaser]* …………………………………………………………………………………………………. ………………………………………………………………………………………………….Whereas ……………………. *[name and address of Supplier]* (hereinafter called “the Supplier”) has undertaken, in pursuance of Contract No. …… dated ……………………… to execute …………………………… *[name of Contract and brief description of Works]* (hereinafter called “the Contract”);And whereas it has been stipulated by you in the said Contract that the Supplier shall furnish you with a Bank Guarantee by a recognized bank for the sum specified therein as security for compliance with his obligations in accordance with the Contract;And whereas we have agreed to give the Supplier such a Bank Guarantee;Now therefore we hereby affirm that we are the Guarantor and responsible to you, on behalf of the Supplier, up to a total of \*…………….. *[amount of Guarantee]* ……………………… *[amount in words]*, such sum being payable in the types and proportions of currencies in which the Contract Price is payable, and we undertake to pay you, upon your first written demand and without cavil or argument, any sum or sums within the limits of ……………… *[amount of Guarantee]* as aforesaid without your needing to prove or to show grounds or reasons for your demand for the sum specified therein.

|  |
| --- |
| \*An amount is to be inserted by the Guarantor, representing the percentage of the Contract Price specified in the Contract, in Maldivian Rufiyaa. |

We hereby waive the necessity of your demanding the said debt from the Supplier before presenting us with the demand.We further agree that no change or addition to or other modification of the terms of the Contract or of the Works to be performed there under or of any of the Contract documents which may be made between you and the Supplier shall in any way release us from any liability under this Guarantee, and we hereby waive notice of any such change, addition, or modification.This Guarantee shall be valid until the date of issue of the Defects Correction Certificate. Signature and seal of the Guarantor ……………………….. Name of Bank …………………………………….. Address …………………………………….. …………………………………….. …………………………………….. Date ………………………………………

|  |
| --- |
| **ޖަދުވަލު – 9** |
| **އެޑްވާންސް ޕޭމަންޓް ގެރެންޓީ** |
| Form of Bank Guarantee for Advance PaymentTo: …………………………………………………………………………………………………. *[name & address of Purchaser*] ………………………………………………………………………………………………….. ………………………………………………………………………………………………… *[name of Contract]*Gentlemen:In accordance with the provisions of the Conditions of Contract, of the above-mentioned Contract, ………… ………………………………………………………………………….*[name and address of Supplier]* (hereinafter called “the Supplier”) shall deposit with ……………………………… ……… ………… …… ……………………….. *[name of Purchaser]* a Bank Guarantee to guarantee his proper and faithful performance under the said Clause of the Contract in an amount of ……….*[amount of Guarantee]* ………………………………………………………………..*[amount in words]*.We, the ………………… …………………………………… …………………………………… *[Bank or Financial Institution]*, as instructed by the Supplier, agree unconditionally and irrevocably to guarantee as primary obligator and not as Surety merely, the payment to …………………………………………………. *[name of Purchaser]* on his first demand without whatsoever right of objection on our part and without his first claim to the Supplier, in the amount not exceeding \*……………………….. ………………………………… [*amount of Guarantee]……… ……………………………………………………………………… [amount in words]*.We further agree that no change or addition to or other modification of the terms of the Contract or of Works to be performed there under or of any of the Contract documents which may be made between ………………………… ………… …………………….…….*[name of Purchaser]* and the Supplier, shall in any way release us from any liability under this Guarantee, and we hereby waive notice of any such change, addition, or modification.

|  |
| --- |
|  \* An amount is to be inserted by the Bank or Financial Institution representing the amount of the Advance Payment, in Maldivian Rufiyaa. |

This Guarantee shall remain valid and in full effect from the date of the advance payment under the Contract until ………………………………………………*[name of Purchaser]* receives full repayment of the same amount from the Supplier. Yours truly,signature and seal: ………………………………………………………………….. Name & address of bank/institution ……………………………………………….

|  |
| --- |
| **ޖަދުވަލު – 10** |
| **ސްޕެސިފިކޭޝަން** |

Bidders are required to fill the Bidder’s specification form and if any information in the specification form are missing or does not meet the requirement specified by the Ministry of Education, the Bidder’s proposed bid document will be disqualified.

| LOT 1 | Supply, Installation, Configuration, and Training for Computing Expansion And Backup Infrastructure Upgrade |
| --- | --- |
| # | Minimum Requirements | Quantity | Specification of the proposed item and relevant parts number |
| 1.1 | **Primary Hosting Server and Storage Expansion** | **01 Bundle** |  |
| 1.1.1 | Brand  |  |
| 1.1.2 | Model |  |
| 1.1.3 | 02 Node x Hyperconverge Appliance in a fully integrated system |  |
| 1.1.4 | Processor: Dual Intel Xeon-Gold 5220R (2.2GHz/24-core/150W) per node |  |
| 1.1.5 | Memory: 384GB RDIMM DDR4-2933 Registered Memory per node |  |
| 1.1.6 | The appliance shall support on Demand Scale-in and Scale-out Architecture |  |
| 1.1.7 | The appliance shall have always-on deduplication and compression from day one including any appropriate license |  |
| 1.1.8 | The appliance shall include built-in resiliency, backup, and disaster recovery for enterprise-grade data protection |  |
| 1.1.9 | Storage: 12 x 1.92TB MU SSD, 2 x 300GB SAS 10K HDD per node |  |
| 1.1.10 | RAID Controller with 2GB Cache and Battery for Cache Protection per node |  |
| 1.1.11 | Redundant hot plug 1600W Power Supply per node |  |
| 1.1.12 | 02 x 10/25Gb dual port SFP28 Network Adapter with transceivers |  |
| 1.1.13 | Embedded 1 x out-of-band management to simplify remote management |  |
| 1.1.14 | Server bezel kit and rack mount railing kit |  |
| 1.1.15 | The appliance shall include enterprise server remote management software License |  |
| 1.1.16 | The system shall be configured as a single cluster |  |
| 1.1.17 | The cluster shall be configured for N+1 high availability |  |
| 1.1.18 | The system shall dedupe and compress all data at inception |  |
| 1.1.19 | Deduplication and compression should be global, meaning data replicated to other future clusters is already deduped and compressed |  |
| 1.1.20 | The system should be resilient and should be able to tolerate multiple drive and component failures in a single node |  |
| 1.1.21 | The system shall include individual VM-centric policy-based backup and recovery. All necessary software like backup software licenses shall be included. Backup software shall be licensed for all the sockets in the proposed HCI cluster. |  |
| 1.1.22 | All backups shall be deduped and compressed natively |  |
| 1.1.23 | The system shall have global management that is directly integrated with VMware vCenter |  |
| 1.1.24 | The system shall include integrated cloud based Intelligent management and reporting platform |  |
| 1.1.25 | The cloud based platform shall be able to provide analytics across multiple systems. |  |
| 1.1.26 | The cloud based platform shall have high level dashboards showing data efficiency, performance, and backup data efficiency per cluster, per Virtual Machine (VM), and per host |  |
| 1.1.27 | 05 x VMware vSphere 7 Std for 1 processor with 1-Year Basic Support License |  |
| 1.1.28 | 01 x VMware vCenter Server 7 Std (Per Instance) with 1-Year Basic Support License |  |
| 1.1.29 | 144 x Windows Server 2022 Standard - 2 Core License Pack License |  |
| 1.1.30 | Minimum required certifications:* Original Equipment Manufacturer (OEM) Certified Professional for the proposed Hyperconverged Appliance (minimum one certified person)
* OEM Certified Professional for the proposed Virtual Backup Appliance (minimum one certified person)
* Veeam Certified (minimum one certified person)
* VMware Certified (minimum one certified person)
 |  |
| 1.1.31 | Installation, Configuration, Documentation and Training* Installation and configuration service shall be by vendor certified persons only
* The installation team should consist of minimum one OEM certified person in the proposed HCI solution.
* The allocated persons shall be available onsite for the duration of the installation
* Installation of the HCI Nodes: unpacking the server, inspecting it for damage and installing it according to product specification
* Installation of any additional hardware options
* Physical connection of the product to a LAN or WAN
* Perform maintenance related tasked such as firmware updates and management interface configuration
* Shall be installed and configured as per manufacturer best practice guidelines.
* Requires configuring / migrating any relevant existing settings to the new devices installed.
* Install and configure hypervisor software on each HCI node
* Install and configure HCI software stack
* Install and configure VMware vCenter with integrated HCI management software
* Configure integrated cloud management platform
* Configure the cluster in N+1 HA configuration
* Configure all relevant VMware networking stack ensuring high availability and maximum performance
* Configure inbuilt backup and recovery for local backup
* Plan, design and configure backup policies
* Backup policies should be configured per VM and globally per datastore
* Migrate selected production workload VMs to new HCI with minimal downtime
* On the job training (Minimum 3 IT staff of MoE)
* Entire VMware infrastructure brief: (Data Centre (DC) and Disaster Recovery (DR) site with diagrams if any)
	+ Step by step guide on how to extend VM storage and file server storage using existing storage capacity.
	+ Step by step guide on how to create and managing windows sever VM.
	+ Step by setup guide on how to create VM by using a template
	+ Step by step guide on how to take backup and restore VMs.
	+ Step by step guide on how to create new data store and present the storage to VMs
	+ Step by step guide on how to migrate VMs
	+ Step by step guide on how to troubleshoot VMs
	+ Step by step guide on managing ESXi hosts.
	+ A complete entire network diagram (with IPs and port numbers)
	+ Step by step guide on Infrastructure bringing up and shutdown procedure:
		- Primary site
* All login credentials should be provided
	+ Other relevant user guide (if any)
 |  |
| 1.1.32 | Warranty:* 3-Year Parts, 3-Year Labor, 3-Year Onsite support with Next Business Day (NBD) response
* 9x5 business hour availability and a 2-hour response time
* 24x7 access to online self-serve and self-solve capabilities, 24x7 incident logging
 |  |
| 1.1.33 | Technical Support: 3-Year local technical support by OEM certified persons |  |
| 1.2 | **Central Management and Backup Server** | **01 Bundle** |  |
| 1.2.1 | Brand |  |
| 1.2.2 | Model |  |
| 1.2.3 | 2U Rack mountable server with 4xLFF slots |  |
| 1.2.4 | 01 x Intel Xeon-Silver 4310 2.1GHz 12-core 120W Processor |  |
| 1.2.5 | 04 x 32GB (1x32GB) Dual Rank x4 DDR4-3200 Registered Memory |  |
| 1.2.6 | 02 x 480GB NVMe M.2 SSD boot drive with RAID1 |  |
| 1.2.7 | 08 x 6TB SATA 6G 7.2K LFF HDD |  |
| 1.2.8 | 01 x HW RAID Controller: 8 Internal Lanes, 2GB Cache, 12G SAS Controller |  |
| 1.2.9 | 01 x Ethernet 10Gb dual port SFP+ Adapter including transceivers |  |
| 1.2.10 | 02 x 800W Hot Plug Low Halogen Power Supply |  |
| 1.2.11 | 01 x Server Remote management license |  |
| 1.2.12 | 01 x Server bezel kit and rack mount railing kit |  |
| 1.2.13 | Shall include high-performance software defined virtual backup appliance license |  |
| 1.2.14 | The virtual backup appliance shall be scalable to 500TB of usable capacity |  |
| 1.2.15 | The virtual backup appliance shall support and include license for data at rest and data in flight encryption |  |
| 1.2.16 | The virtual backup appliance shall include at minimum 36TB perpetual capacity license |  |
| 1.2.17 | The virtual backup appliance shall include perpetual deduplication and compression license |  |
| 1.2.18 | The virtual backup appliance shall have a minimum of 4TB/hr backup performance |  |
| 1.2.19 | Veeam Backup & Replication Universal License. 1 Year Subscription (40 VM license) |  |
| 1.2.20 | Minimum required certifications:* OEM Certified Professional for the proposed Virtual Backup Appliance (minimum one certified person)
* Veeam Certified (minimum one certified person)
 |  |
| 1.2.21 | Installation, Configuration, Documentation and Training* Shall be deployed by vendor certified persons only
* The installation team should consist of minimum one OEM certified professional person in the proposed virtual backup appliance and one OEM certified person for Veeam Backup.
* The allocated person(s) should be available onsite for the duration of the installation
* Plan and design external and long term backup and recovery policies as per industry best practices
* Configure backup and recovery policies for all production workload
* Configure virtual backup appliance for long term archiving
* Isolate and secure backup infrastructure
* Configure replication policies on all existing production workloads for continuous data protection
* Demonstrate and verify backup and recovery
* Requires to configure/ migrate any relevant existing settings to the new device installed as per manufacturer best practice guidelines.
* On the job training (Minimum 3 IT staff of MoE)
* Configuration documentation:
	+ All login credentials should be provided
	+ Veeam backup and recovery user guide
	+ Other relevant user guide (if any)
 |  |
| 1.2.22 | Warranty:* 3-Year Parts, 3-Year Labor, 3-Year Onsite support with NBD response
* 9x5 business hour availability and a 2-hour response time
* 24x7 access to online self-serve and self-solve capabilities, 24x7 incident logging
 |  |
| 1.2.23 | Technical Support: 3-Year local technical support by OEM certified persons |  |
| 1.3 | **Primary Site Next Generation Network Security Appliance** | **01 Bundle** |  |
| 1.3.1 | Brand |  |  |
| 1.3.2 | Model |  |  |
| 1.3.3 | The device shall have minimum the following interfaces and modules* 8x1 Gig SFP
* 16x1 Gig RJ-45 ports
* 2x10 Gig SFP+ ports
* 1 x Console Port

1 x 480GB SSD on board storage |  |  |
| 1.3.4 | The device should support minimum 25Gbps firewall throughput |  |  |
| 1.3.5 | The device shall support minimum 5Gbps IPS throughput |  |  |
| 1.3.6 | The device shall support minimum 3.2Gbps NGFW throughput |  |  |
| 1.3.7 | The device shall support minimum 3Gbps Threat Protection throughput |  |  |
| 1.3.8 | The device shall support minimum 2Gbps SSL VPN throughput |  |  |
| 1.3.9 | The device shall have support minimum 2.9 Million Concurrent TCP Sessions |  |  |
| 1.3.10 | The device shall support active-active or active-passive high availability configuration |  |  |
| 1.3.11 | The device shall have redundant power supply unit |  |  |
| 1.3.12 | Form factor: 1RU, rack mounting accessories shall be included |  |  |
| 1.3.13 | The proposed next generation firewall should be an enterprise grade firewall from a manufacturer listed as Leader in the 2020 or 2021 Gartner Magic Quadrant for Network Firewalls. Should submit relevant Gartner’s magic quadrant report |  |  |
| 1.3.14 | The appliance shall support intercepting SSL traffic for Security Filtering. |  |  |
| 1.3.15 | The appliance shall be able to perform the security functionalities of Web Filter, Application Control, IPS, and Antivirus. |  |  |
| 1.3.16 | The appliance shall support OSPF, BGP, static, IGMP v1/v2, PIM, VRRP, BFD protocol  |  |  |
| 1.3.17 | The appliance should support 802.1Q, sub interface, bridge domains, Inter VLAN routing.  |  |  |
| 1.3.18 | The appliance should support policy based routing, Application aware routing, performance based routing.  |  |  |
| 1.3.19 | The appliance shall support various traffic load balancing mechanism between multiple transport.  |  |  |
| 1.3.20 | The appliance should support QoS based on layer-7 application  |  |  |
| 1.3.21 | The appliance should support NAT/PAT for direct internet access or cloud access  |  |  |
| 1.3.22 | The appliance architecture should have dedicated CPU for security processing apart from the main central processing units (CPUs). |  |  |
| 1.3.23 | The appliance should identify thousands of applications inside network traffic for deep inspection and granular policy enforcement |  |  |
| 1.3.24 | The appliance should protect against malware, exploits, and malicious websites in both encrypted and non-encrypted traffic |  |  |
| 1.3.25 | The appliance should prevent and detect against known and unknown attacks using continuous threat intelligence backed by dedicated global security services |  |  |
| 1.3.26 | The appliance shall support automatically blocking threats on decrypted traffic using the Industry’s standard SSL inspection |  |  |
| 1.3.27 | The appliance shall support blocking and controlling web access based on user or user groups across URL’s and domains |  |  |
| 1.3.28 | The appliance shall support Block DNS requests against malicious domains |  |  |
| 1.3.29 | The appliance shall support Multi-layered advanced protection against zero-day malware threats delivered over the web |  |  |
| 1.3.30 | The appliance shall include a management console that is effective, simple to use, and provides comprehensive network automation and visibility |  |  |
| 1.3.31 | The appliance shall provide converged networking and security into a secure, simple to manage architecture with a single focal point for management and configuration for LAN devices such as Network Switches and Wireless Access Points. |  |  |
| 1.3.32 | Security Subscription:* 1-Year Security Subscription - Web Filtering, Malware Protection, IPS, Antispam, Antivirus, Botnet, Virus Outbreak Protection, Application Control, Sandbox
* 1-Year Support Subscription: 24x7 Support, Hardware Replacement, Firmware Upgrades
 |  |  |
| 1.3.33 | Minimum required certifications:* Cisco CCNA Certified for Routing and Switching Certified (minimum one certified person)
* Cisco CCNA and CCNP Certified for Security Certified (minimum one certified person)
* OEM Certified Professional for the proposed Network Security Appliance (minimum one certified person)
 |  |  |
| 1.3.34 | Installation, Configuration, Documentation and Training* Shall be deployed by vendor certified persons only
* The installation team should consist of minimum
	+ 01 x OEM certified person for the proposed network security appliance and
	+ 01 x Cisco CCNA and CCNP Certified person
* The allocated person(s) should be available onsite for the duration of the installation
* Design appropriate LAN,WAN, and DMZ security policies.
* Configure application control policies
* Configure AV and Web filtering policies
* Configure antispam filtering
* Configure malware protection policies
* Configure IPS policies
* Configure traffic shaping and ISP WAN load balancing
* Network segmentation and configure appropriate security policy per segment
* Configure remote access connectivity policies
* Configure DNS filtering policies
* Configure wireless network segmentation and appropriate security polices per segment
* Configure wireless network bandwidth management policies
* Configure security event logging and monitoring
* Configure security event alert notification
* Configure scheduled industry standard security reporting policies
* Requires to configure/ migrate any relevant existing policies and settings to the new device installed as per manufacturer best practice guidelines.
* On the job training (Minimum 3 IT staff of MoE)
* Configuration documentation:
* All login credentials should be provided
* User guide of the security policies configured
* Other relevant user guide (if any)
 |  |  |
| 1.3.35 | Warranty: 1-Year Parts and Service with 24x7 comprehensive support, Hardware Replacement, Firmware Upgrades |  |  |
| 1.3.36 | Technical Support: 1-Year 24x7 on-site technical support services and labor |  |  |
| 1.4 | **Moving of existing MSA at Primary Site to Disaster Recovery Site**  |  |  |
| 1.4.1 | Move the existing SAN storage from Primary Site to DR site:* Install and configure the storage at DR Site with latest firmware upgrades.
* Requires to configure/ migrate any relevant existing settings at DR Site to the moved storage as per manufacturer best practice guidelines.
 |  |  |
| 1.4.2 | Installation, Configuration, Documentation and Training* Move the existing SAN storage from Primary Site to DR site:
	+ Install and configure the storage at DR Site with latest firmware upgrades.
	+ Requires to configure/ migrate any relevant existing settings at DR Site to the moved storage as per manufacturer best practice guidelines.
* On the job training (Minimum 3 IT staff of MoE)
* Entire VMware infrastructure brief of DR Site:
	+ Step by step guide on how to extend VM storage and file server storage using existing storage capacity.
	+ Step by step guide on managing ESXi hosts.
	+ A complete entire network diagram (with IPs and port numbers)
	+ DR site details (Step by step guide)
	+ Step by step guide of Infrastructure bringing up and shutdown procedure:
		- Disaster recovery site
	+ Other relevant user guide (if any)
 |  |  |

 |
|

|  |
| --- |
| **ޖަދުވަލު – 10** |
| **ހުށަހަޅާ ޓެކްނިކަލް ޓީމްގެ މަޢުލޫމާތު، ސީ.ވީ ،އެކްރެޑިޓެޑް ސެޓްފިކެޓްތައް** |

**Team members Information**List all Members in the team as per reqirement in section 7(Team Members Curriculum Vitae and supporting documents should be submitted along with the proposal and this form should be signed and stamped by Tenderer).

|  |  |  |  |
| --- | --- | --- | --- |
| **Team member Name** | **Contact No** | **ID Card No**  | **Qualifications** |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |

**Primary required certificates of the professional(s):** * Cisco CCNA Certified for Routing and Switching Certified
* Cisco CCNA and CCNP Certified for Security Certified
* OEM Certified Professional for the proposed Network Security Appliance
* OEM Certified Professional for the proposed Hyperconverged Appliance
* OEM Certified Professional for the proposed Virtual Backup Appliance
* Veeam Certified
* VMware Certified

**Curriculum Vitae** 1. **Name:**
2. **Education** *[Indicate college/university and other specialized education of staff member, giving names of institutions, degrees obtained, and dates of obtainment]:*
3. **Other Training**
4. **Languages** *[For each language indicate proficiency: good, fair, or poor in speaking, reading, and writing]:*
5. **Experience/ employment record** *[Starting with present position, list in reverse order every employment held since graduation, giving for each employment (see format here below): dates of employment, name of employing organization, positions held.]*

From [Month/Year] – To [Month/Year]:Employer: Positions held:1. **Summary of projects/assignments undertaken/ role**

Name of project/ assignment:Experience classification: General / specificScope of project/ assignment: Role/ Position undertaken: Period of assignment: |

 |
| **ސެކްޝަން - 5**  |
|

|  |
| --- |
| **ކޮންޓްރެކްޓް ޑާޓާ ޝީޓް** |
| **ކޮންޓްރެކްޓާގުޅޭ ރިފަރަންސްތައް** | **ރިފަރަންސް ނަންބަރު** |
| މަސައްކަތުގެ ވެރިފަރާތުގެ މައުލޫމާތުނަން:އެޑްރެސް: | 33.1 |
| މަސައްކަތް ހަވާލުވާފަރާތުގެ މައުލޫމާތުނަން:އެޑްރެސް: | 33.2 |
| މަސައްކަތުގެ މަޢުލޫމާތު: | 33.3 |
| މަސައްކަތުގެ އަގު: | 33.4 |
| އެއްބަސްވުމުގެ މުއްދަތު: | 37 |

 |
|  |
| **ސެކްޝަން- 6**  |
| **އެއްބަސްވުން** |
| މި އެގްރީމަންޓް ކުރެވިފައި ވަނީ، -------------------- (މި އެއްބަސްވުމުގައި މީގެ ފަހުން "ގަންނަފަރާތް") އާއި ------------ (މި އެއްބަސްވުމުގައި މީގެފަހުން "ވިއްކާފަރާތް") އާ ދެމެދު، މީލާދީ ސަނަތުން، ........... ވަނަ އަހަރުގެ ........................ މަހުގެ ....... (..................) ދުވަހު އެވެ.  |
| ދެންފަހެ، ............................ (މި އެއްބަސްވުމުގައި މީގެ ފަހުން "މަސައްކަތްތައް") ކުރުމަށް ގަންނަފަރާތުން ބޭނުންވި ހިނދު، އަދި އެކަމަށްޓަކައި ވިއްކާފަރާތުން ހުށަހަޅާފައިވާ އަންދާސީ ހިސާބު ގަންނަފަރާތުން ޤަބޫލުކުރި ހިނދު، ބުނެވިދިޔަ މަސައްކަތްތައް ވިއްކާފަރާތުން ކުރުމަށާއި، އަދި އެ މަސައްކަތްތައް ފޯރުކޮށްދިނުމުގައި ލިބޭ ގެއްލުމަކަށް ބަދަލު ދޭންޖެހޭނަމަ އެކަމެއް ކުރުމަށް ނިޔަތްގަނެ، އަންނަނިވި ކަންކަމަށް އެއްބަސްވަމެވެ. 1. މި އެއްބަސްވުމުގައި ބަޔާންކޮށްފައިވާ މުސްތަލަޙުތަކާއި އިސްތިލާޙުތައް މާނަކުރުމުގައި "އެއްބަސްވުމުގެ ޝަރުޠުތައް" ގައި އެ މުސްތަލަޙެއް ނުވަތަ އިސްތިލާޙެއް ބޭނުންކޮށްފައިވާ ގޮތަށް ބަލަންވާނެއެވެ. އަދި އެއީ، މި އެއްބަސްވުމުގެ ބައެއްގެ ގޮތުގައި ބެލެވޭނެއެވެ. 2. މި އެއްބަސްވުމުގައި ކަނޑައަޅާފައިވާ އަގަށް، އަދި އެ އަގު ދެއްކުމަށް ކަނޑައަޅާފައިވާގޮތަށް ރިޢާޔަތްކޮށް އެއްބަސްވުމުގެދަށުން ކުރަންޖެހޭ މަސައްކަތްތައް ކުރުމަށާއި، އަދި އެ މަސައްކަތްކުރުމުގައި މި އެއްބަސްވުމުގެ ޝަރުޠުތަކާ އެއްގޮތްނުވާ މަސައްކަތްތަކަށް ލިބިދޭންޖެހޭ ބަދަލު ދިނުމަށް ވިއްކާފަރާތުން އެއްބަސްވެއެވެ. 3. މި އެއްބަސްވުމުގައި ކަނޑައަޅާފައިވާ މަސައްކަތްތައް ކުރިއަށް ގެންގޮސް ނިންމުމާއި، އަދި އިސްލާޙު ކުރަންޖެހޭ މަސައްކަތްތައް އެއްބަސްވުމުގެ ޝަރުޠުތަކާއި އެއްގޮތަށް އިސްލާޙުކުރުމާ ގުޅިގެން ވިއްކާފަރާތަށް ލިބިދޭންޖެހޭ މަސައްކަތުގެ އަގު ނުވަތަ އެއްބަސްވުމުގެ ޝަރުޠުތަކާ އެއްގޮތްވާ ގޮތުގެމަތިން ވިއްކާފަރާތުން ކޮށްނިންމާ މަސައްކަތްތަކަށް ދޭންޖެހޭ އެންމެހާ ފައިސާ ވިއްކާފަރާތަށް ދިނުމަށް ގަންނަފަރާތުން އެއްބަސްވެއެވެ.  |
| މި އެއްބަސްވުން އެކުލެވިގެންވަނީ ބީލަމާ ގުޅިގެން ދެވުނު މަޢުލޫމާތާއި، އެއްބަސްވުމުގެ އާންމު މާއްދާތަކާއި، މަސައްކަތް ހަވާލުވި ފަރާތުން ހުށަހަޅާފައިވާ ޕްރޮޕޯސަލްގެ މައްޗަށެވެ. |
| މި އެއްބަސްވުމަކީ، މި އެއްބަސްވުމުގެ އެންމެހައި މާއްދާތަކަށް އިޙްތިރާމްކުރުމާއި، އެއްބަސްވުމުގައި ބަޔާންކުރާ މަޤްޞަދުތައް ޙާޞިލްކުރުމަށްޓަކައި، ދެފަރާތުން މިއެއްބަސްވުމުގެ މުއްދަތަށް އެއްބަސްވުން ދެމެހެއްޓުމުގެ ނިޔަތުގައި ތިރީގައިވާ މީހުން ހެކިކޮށް، ދެފަރާތުގެ ފުރިހަމަ އިޚްތިޔާރާ އެކު ސޮއިކޮށްފައިވާ ޞައްޙަ އެއްބަސްވުމެކެވެ. |

|  |  |
| --- | --- |
| **މަސައްކަތުގެ ވެރިފަރާތް:**  | **މަސައްކަތާ ހަވާލުވާ ފަރާތް:** |
| ސޮއި: | ސޮއި: |
| ނަން:  | ނަން:  |
| މަޤާމް:  | މަޤާމް:  |
| ތައްގަނޑު:  | ތައްގަނޑު:  |
| **ހެކިން:**  | **ހެކިން:** |
| ސޮއި: | ސޮއި: |
| ނަން:  | ނަން:  |
| މަޤާމް:  | މަޤާމް:  |
| އައި.ޑީ#: | އައި.ޑީ#: |
| **މަސައްކަތުގެ ވެރިފަރާތުން ސްޕަވައިޒު ކުރާނީ**  | **މަސައްކަތް ހަވާލުވާ ފަރާތުން ސްޕަވައިޒު ކުރާނީ**  |
| ސޮއި: | ސޮއި: |
| ނަން:  | ނަން:  |
| މަޤާމް:  | މަޤާމް:  |
| އައި.ޑީ#: | އައި.ޑީ#: |
| ގުޅޭނެ ނަންބަރު: | ގުޅޭނެ ނަންބަރު: |
| އީމެއިލް އެޑްރެސް: | އީމެއިލް އެޑްރެސް: |

|  |
| --- |
| **ސެކްޝަން - 7** |
| **ބޭނުންވާ ޚިދުމަތް/ތަކެތި/މަސައްކަތުގެ ތަފްސީލް**މިމިނސްޓްރީގެ ޑާޓާސެންޓަރ އަޕްގުރޭޑުކޮށް އެކްސްޕޭންޑް ކުރުން

| LOT 1 | Supply, Installation, Configuration, and Training for Computing Expansion And Backup Infrastructure Upgrade |
| --- | --- |
| # | Minimum Requirements | Quantity |
| 1.1 | **Primary Hosting Server and Storage Expansion** | **01 Bundle** |
| 1.1.1 | Brand  |
| 1.1.2 | Model |
| 1.1.3 | 02 Node x Hyperconverge Appliance in a fully integrated system |
| 1.1.4 | Processor: Dual Intel Xeon-Gold 5220R (2.2GHz/24-core/150W) per node |
| 1.1.5 | Memory: 384GB RDIMM DDR4-2933 Registered Memory per node |
| 1.1.6 | The appliance shall support on Demand Scale-in and Scale-out Architecture |
| 1.1.7 | The appliance shall have always-on deduplication and compression from day one including any appropriate license |
| 1.1.8 | The appliance shall include built-in resiliency, backup, and disaster recovery for enterprise-grade data protection |
| 1.1.9 | Storage: 12 x 1.92TB MU SSD, 2 x 300GB SAS 10K HDD per node |
| 1.1.10 | RAID Controller with 2GB Cache and Battery for Cache Protection per node |
| 1.1.11 | Redundant hot plug 1600W Power Supply per node |
| 1.1.12 | 02 x 10/25Gb dual port SFP28 Network Adapter with transceivers |
| 1.1.13 | Embedded 1 x out-of-band management to simplify remote management |
| 1.1.14 | Server bezel kit and rack mount railing kit |
| 1.1.15 | The appliance shall include enterprise server remote management software License |
| 1.1.16 | The system shall be configured as a single cluster |
| 1.1.17 | The cluster shall be configured for N+1 high availability |
| 1.1.18 | The system shall dedupe and compress all data at inception |
| 1.1.19 | Deduplication and compression should be global, meaning data replicated to other future clusters is already deduped and compressed |
| 1.1.20 | The system should be resilient and should be able to tolerate multiple drive and component failures in a single node |
| 1.1.21 | The system shall include individual VM-centric policy-based backup and recovery. All necessary software like backup software licenses shall be included. Backup software shall be licensed for all the sockets in the proposed HCI cluster. |
| 1.1.22 | All backups shall be deduped and compressed natively |
| 1.1.23 | The system shall have global management that is directly integrated with VMware vCenter |
| 1.1.24 | The system shall include integrated cloud based Intelligent management and reporting platform |
| 1.1.25 | The cloud based platform shall be able to provide analytics across multiple systems. |
| 1.1.26 | The cloud based platform shall have high level dashboards showing data efficiency, performance, and backup data efficiency per cluster, per Virtual Machine (VM), and per host |
| 1.1.27 | 05 x VMware vSphere 7 Std for 1 processor with 1-Year Basic Support License |
| 1.1.28 | 01 x VMware vCenter Server 7 Std (Per Instance) with 1-Year Basic Support License |
| 1.1.29 | 144 x Windows Server 2022 Standard - 2 Core License Pack License |
| 1.1.30 | Minimum required certifications:* Original Equipment Manufacturer (OEM) Certified Professional for the proposed Hyperconverged Appliance (minimum one certified person)
* OEM Certified Professional for the proposed Virtual Backup Appliance (minimum one certified person)
* Veeam Certified (minimum one certified person)
* VMware Certified (minimum one certified person)
 |
| 1.1.31 | Installation, Configuration, Documentation and Training* Installation and configuration service shall be by vendor certified persons only
* The installation team should consist of minimum one OEM certified person in the proposed HCI solution.
* The allocated persons shall be available onsite for the duration of the installation
* Installation of the HCI Nodes: unpacking the server, inspecting it for damage and installing it according to product specification
* Installation of any additional hardware options
* Physical connection of the product to a LAN or WAN
* Perform maintenance related tasked such as firmware updates and management interface configuration
* Shall be installed and configured as per manufacturer best practice guidelines.
* Requires configuring / migrating any relevant existing settings to the new devices installed.
* Install and configure hypervisor software on each HCI node
* Install and configure HCI software stack
* Install and configure VMware vCenter with integrated HCI management software
* Configure integrated cloud management platform
* Configure the cluster in N+1 HA configuration
* Configure all relevant VMware networking stack ensuring high availability and maximum performance
* Configure inbuilt backup and recovery for local backup
* Plan, design and configure backup policies
* Backup policies should be configured per VM and globally per datastore
* Migrate selected production workload VMs to new HCI with minimal downtime
* On the job training (Minimum 3 IT staff of MoE)
* Entire VMware infrastructure brief: (Data Centre (DC) and Disaster Recovery (DR) site with diagrams if any)
	+ Step by step guide on how to extend VM storage and file server storage using existing storage capacity.
	+ Step by step guide on how to create and managing windows sever VM.
	+ Step by setup guide on how to create VM by using a template
	+ Step by step guide on how to take backup and restore VMs.
	+ Step by step guide on how to create new data store and present the storage to VMs
	+ Step by step guide on how to migrate VMs
	+ Step by step guide on how to troubleshoot VMs
	+ Step by step guide on managing ESXi hosts.
	+ A complete entire network diagram (with IPs and port numbers)
	+ Step by step guide on Infrastructure bringing up and shutdown procedure:
		- Primary site
* All login credentials should be provided
	+ Other relevant user guide (if any)
 |
| 1.1.32 | Warranty:* 3-Year Parts, 3-Year Labor, 3-Year Onsite support with Next Business Day (NBD) response
* 9x5 business hour availability and a 2-hour response time
* 24x7 access to online self-serve and self-solve capabilities, 24x7 incident logging
 |
| 1.1.33 | Technical Support: 3-Year local technical support by OEM certified persons |
| 1.2 | **Central Management and Backup Server** | **01 Bundle** |
| 1.2.1 | Brand |
| 1.2.2 | Model |
| 1.2.3 | 2U Rack mountable server with 4xLFF slots |
| 1.2.4 | 01 x Intel Xeon-Silver 4310 2.1GHz 12-core 120W Processor |
| 1.2.5 | 04 x 32GB (1x32GB) Dual Rank x4 DDR4-3200 Registered Memory |
| 1.2.6 | 02 x 480GB NVMe M.2 SSD boot drive with RAID1 |
| 1.2.7 | 08 x 6TB SATA 6G 7.2K LFF HDD |
| 1.2.8 | 01 x HW RAID Controller: 8 Internal Lanes, 2GB Cache, 12G SAS Controller |
| 1.2.9 | 01 x Ethernet 10Gb dual port SFP+ Adapter including transceivers |
| 1.2.10 | 02 x 800W Hot Plug Low Halogen Power Supply |
| 1.2.11 | 01 x Server Remote management license |
| 1.2.12 | 01 x Server bezel kit and rack mount railing kit |
| 1.2.13 | Shall include high-performance software defined virtual backup appliance license |
| 1.2.14 | The virtual backup appliance shall be scalable to 500TB of usable capacity |
| 1.2.15 | The virtual backup appliance shall support and include license for data at rest and data in flight encryption |
| 1.2.16 | The virtual backup appliance shall include at minimum 36TB perpetual capacity license |
| 1.2.17 | The virtual backup appliance shall include perpetual deduplication and compression license |
| 1.2.18 | The virtual backup appliance shall have a minimum of 4TB/hr backup performance |
| 1.2.19 | Veeam Backup & Replication Universal License. 1 Year Subscription (40 VM license) |
| 1.2.20 | Minimum required certifications:* OEM Certified Professional for the proposed Virtual Backup Appliance (minimum one certified person)
* Veeam Certified (minimum one certified person)
 |
| 1.2.21 | Installation, Configuration, Documentation and Training* Shall be deployed by vendor certified persons only
* The installation team should consist of minimum one OEM certified professional person in the proposed virtual backup appliance and one OEM certified person for Veeam Backup.
* The allocated person(s) should be available onsite for the duration of the installation
* Plan and design external and long term backup and recovery policies as per industry best practices
* Configure backup and recovery policies for all production workload
* Configure virtual backup appliance for long term archiving
* Isolate and secure backup infrastructure
* Configure replication policies on all existing production workloads for continuous data protection
* Demonstrate and verify backup and recovery
* Requires to configure/ migrate any relevant existing settings to the new device installed as per manufacturer best practice guidelines.
* On the job training (Minimum 3 IT staff of MoE)
* Configuration documentation:
	+ All login credentials should be provided
	+ Veeam backup and recovery user guide
	+ Other relevant user guide (if any)
 |
| 1.2.22 | Warranty:* 3-Year Parts, 3-Year Labor, 3-Year Onsite support with NBD response
* 9x5 business hour availability and a 2-hour response time
* 24x7 access to online self-serve and self-solve capabilities, 24x7 incident logging
 |
| 1.2.23 | Technical Support: 3-Year local technical support by OEM certified persons |
| 1.3 | **Primary Site Next Generation Network Security Appliance** | **01 Bundle** |
| 1.3.1 | Brand |  |
| 1.3.2 | Model |  |
| 1.3.3 | The device shall have minimum the following interfaces and modules* 8x1 Gig SFP
* 16x1 Gig RJ-45 ports
* 2x10 Gig SFP+ ports
* 1 x Console Port

1 x 480GB SSD on board storage |  |
| 1.3.4 | The device should support minimum 25Gbps firewall throughput |  |
| 1.3.5 | The device shall support minimum 5Gbps IPS throughput |  |
| 1.3.6 | The device shall support minimum 3.2Gbps NGFW throughput |  |
| 1.3.7 | The device shall support minimum 3Gbps Threat Protection throughput |  |
| 1.3.8 | The device shall support minimum 2Gbps SSL VPN throughput |  |
| 1.3.9 | The device shall have support minimum 2.9 Million Concurrent TCP Sessions |  |
| 1.3.10 | The device shall support active-active or active-passive high availability configuration |  |
| 1.3.11 | The device shall have redundant power supply unit |  |
| 1.3.12 | Form factor: 1RU, rack mounting accessories shall be included |  |
| 1.3.13 | The proposed next generation firewall should be an enterprise grade firewall from a manufacturer listed as Leader in the 2020 or 2021 Gartner Magic Quadrant for Network Firewalls. Should submit relevant Gartner’s magic quadrant report |  |
| 1.3.14 | The appliance shall support intercepting SSL traffic for Security Filtering. |  |
| 1.3.15 | The appliance shall be able to perform the security functionalities of Web Filter, Application Control, IPS, and Antivirus. |  |
| 1.3.16 | The appliance shall support OSPF, BGP, static, IGMP v1/v2, PIM, VRRP, BFD protocol  |  |
| 1.3.17 | The appliance should support 802.1Q, sub interface, bridge domains, Inter VLAN routing.  |  |
| 1.3.18 | The appliance should support policy based routing, Application aware routing, performance based routing.  |  |
| 1.3.19 | The appliance shall support various traffic load balancing mechanism between multiple transport.  |  |
| 1.3.20 | The appliance should support QoS based on layer-7 application  |  |
| 1.3.21 | The appliance should support NAT/PAT for direct internet access or cloud access  |  |
| 1.3.22 | The appliance architecture should have dedicated CPU for security processing apart from the main central processing units (CPUs). |  |
| 1.3.23 | The appliance should identify thousands of applications inside network traffic for deep inspection and granular policy enforcement |  |
| 1.3.24 | The appliance should protect against malware, exploits, and malicious websites in both encrypted and non-encrypted traffic |  |
| 1.3.25 | The appliance should prevent and detect against known and unknown attacks using continuous threat intelligence backed by dedicated global security services |  |
| 1.3.26 | The appliance shall support automatically blocking threats on decrypted traffic using the Industry’s standard SSL inspection |  |
| 1.3.27 | The appliance shall support blocking and controlling web access based on user or user groups across URL’s and domains |  |
| 1.3.28 | The appliance shall support Block DNS requests against malicious domains |  |
| 1.3.29 | The appliance shall support Multi-layered advanced protection against zero-day malware threats delivered over the web |  |
| 1.3.30 | The appliance shall include a management console that is effective, simple to use, and provides comprehensive network automation and visibility |  |
| 1.3.31 | The appliance shall provide converged networking and security into a secure, simple to manage architecture with a single focal point for management and configuration for LAN devices such as Network Switches and Wireless Access Points. |  |
| 1.3.32 | Security Subscription:* 1-Year Security Subscription - Web Filtering, Malware Protection, IPS, Antispam, Antivirus, Botnet, Virus Outbreak Protection, Application Control, Sandbox
* 1-Year Support Subscription: 24x7 Support, Hardware Replacement, Firmware Upgrades
 |  |
| 1.3.33 | Minimum required certifications:* Cisco CCNA Certified for Routing and Switching Certified (minimum one certified person)
* Cisco CCNA and CCNP Certified for Security Certified (minimum one certified person)
* OEM Certified Professional for the proposed Network Security Appliance (minimum one certified person)
 |  |
| 1.3.34 | Installation, Configuration, Documentation and Training* Shall be deployed by vendor certified persons only
* The installation team should consist of minimum
	+ 01 x OEM certified person for the proposed network security appliance and
	+ 01 x Cisco CCNA and CCNP Certified person
* The allocated person(s) should be available onsite for the duration of the installation
* Design appropriate LAN,WAN, and DMZ security policies.
* Configure application control policies
* Configure AV and Web filtering policies
* Configure antispam filtering
* Configure malware protection policies
* Configure IPS policies
* Configure traffic shaping and ISP WAN load balancing
* Network segmentation and configure appropriate security policy per segment
* Configure remote access connectivity policies
* Configure DNS filtering policies
* Configure wireless network segmentation and appropriate security polices per segment
* Configure wireless network bandwidth management policies
* Configure security event logging and monitoring
* Configure security event alert notification
* Configure scheduled industry standard security reporting policies
* Requires to configure/ migrate any relevant existing policies and settings to the new device installed as per manufacturer best practice guidelines.
* On the job training (Minimum 3 IT staff of MoE)
* Configuration documentation:
* All login credentials should be provided
* User guide of the security policies configured
* Other relevant user guide (if any)
 |  |
| 1.3.35 | Warranty: 1-Year Parts and Service with 24x7 comprehensive support, Hardware Replacement, Firmware Upgrades |  |
| 1.3.36 | Technical Support: 1-Year 24x7 on-site technical support services and labor |  |
| 1.4 | **Moving of existing MSA at Primary Site to Disaster Recovery Site**  |  |
| 1.4.1 | Move the existing SAN storage from Primary Site to DR site:* Install and configure the storage at DR Site with latest firmware upgrades.
* Requires to configure/ migrate any relevant existing settings at DR Site to the moved storage as per manufacturer best practice guidelines.
 |  |
| 1.4.2 | Installation, Configuration, Documentation and Training* Move the existing SAN storage from Primary Site to DR site:
	+ Install and configure the storage at DR Site with latest firmware upgrades.
	+ Requires to configure/ migrate any relevant existing settings at DR Site to the moved storage as per manufacturer best practice guidelines.
* On the job training (Minimum 3 IT staff of MoE)
* Entire VMware infrastructure brief of DR Site:
	+ Step by step guide on how to extend VM storage and file server storage using existing storage capacity.
	+ Step by step guide on managing ESXi hosts.
	+ A complete entire network diagram (with IPs and port numbers)
	+ DR site details (Step by step guide)
	+ Step by step guide of Infrastructure bringing up and shutdown procedure:
		- Disaster recovery site
	+ Other relevant user guide (if any)
 |  |

|  |  |
| --- | --- |
| # | General Technical Requirements |
| 1 | **Minimum Service Level requirements:**1. The support service vendor should provide the contact number of a single point of contact to facilitate immediate contact by client’s representative and he or she shall be responsible to liaise with all vendors for rectification of faults within the Next Business Day.
2. Defective equipment shall be replaced by the bidder at his own cost including the cost of transport if any;
3. The support service vendor shall provide all normal toolkit and test equipment needed for the maintenance of the hardware to their engineers.
4. System maintenance and support services will include the following activities.
* 24 x 7 on-line Support.
* Patch updating and major / minor software version upgrading support.
* Phone/ Email TAC support must be provided during support period
* Issue resolution / Onsite Visits within 1 hour of hardware failures reported
* Local TAC support plan must be maintained by the Bidder for the maintenance period.
1. After installation and deployment of each component, the support service vendor is required to provide written confirmation to the Ministry that the part/ component installation and configuration have been completed.
 |
| 2 | **Maintenance Support Services including on-site Technical Support:** * On-site hardware repair/replace and maintenance support service should be delivered by experienced OEM Certified person
* On-site diagnostics and repair service should be delivered by experienced OEM Certified person
* Service summary report shall be provided after each work performed including recommendations for optimal performance
* Maintenance Support Person should check and ensure the systems are with the most recent firmware version.
* During each maintenance visit, field service professionals should run tests to verify our systems are functioning correctly in all operational modes
* Replacements of parts; labour; travels & accommodation and components should be included as per applicable warranty of the relevant system
* The support service vendor shall maintain critical parts locally in Male’ to provide after sale support.
* It is mandatory that the support service vendor should maintain the required support technical team as deemed as suited based on the requirements and milestones. The support service vendor MUST have full time Certified Professional(s)/ Person(s) under its payroll.

Primary required certificates of the professional(s): * Cisco CCNA Certified for Routing and Switching Certified
* Cisco CCNA and CCNP Certified for Security Certified
* OEM Certified Professional for the proposed Network Security Appliance
* OEM Certified Professional for the proposed Hyperconverged Appliance
* OEM Certified Professional for the proposed Virtual Backup Appliance
* Veeam Certified
* VMware Certified

The vendor shall submit the following documents:* Certifications copy of the relevant training
* ID card OR Passport Copy of the certified person/ personnel
 |

**އަގު ހުށަހަޅާނެގޮތުގެ ނަމޫނާ:**

|  |
| --- |
| LOT 1: Supply, Installation, Configuration, and Training for Computing Expansion And Backup Infrastructure Upgrade |
| **#** | **Item Description** | **Quantity** | **Unit Price (MVR)** | **Extended Price (MVR)** |
| 1.1 | Primary Hosting Server and Storage Expansion | 1 Bundle |  |  |
| 1.2 | Central Management and Backup Server | 1 Bundle |  |  |
| 1.3 | Primary Site Next Generation Network Security Appliance | 1 Bundle |  |  |
| **Sub Total** |  |
| **GST 6%** |  |
| **Net Total** |  |

 |